lwIP 2.1.0 Lightweight IP stack

Macros | Functions
autoip.c File Reference
`#include "lwip/opt.h"`
`#include "lwip/mem.h"`
`#include "lwip/ip_addr.h"`
`#include "lwip/netif.h"`
`#include "lwip/autoip.h"`
`#include "lwip/etharp.h"`
`#include "lwip/prot/autoip.h"`
`#include <string.h>`

## Macros
#define | LWIP_AUTOIP_RAND(netif)
#define | LWIP_AUTOIP_CREATE_SEED_ADDR(netif)

## Functions
void | autoip_set_struct (struct netif *netif, struct autoip *autoip)
err_t | autoip_start (struct netif *netif)
void | autoip_network_changed (struct netif *netif)
err_t | autoip_stop (struct netif *netif)
void | autoip_tmr (void)
void | autoip_arp_reply (struct netif *netif, struct etharp_hdr *hdr)
u8_t | autoip_supplied_address (const struct netif *netif)

## Detailed Description

AutoIP Automatic LinkLocal IP Configuration

This is a AutoIP implementation for the lwIP TCP/IP stack. It aims to conform with RFC 3927.

## Macro Definition Documentation

## ◆ LWIP_AUTOIP_CREATE_SEED_ADDR

#define LWIP_AUTOIP_CREATE_SEED_ADDR | ( |  | netif | ) |

Value:
lwip_htonl(AUTOIP_RANGE_START + ((u32_t)(((u8_t)(netif->hwaddr[4])) | \
((u32_t)((u8_t)(netif->hwaddr[5]))) << 8)))
netif::hwaddr
u8_t hwaddr[6U]
Definition: netif.h:341
lwip_htonl
u32_t lwip_htonl(u32_t n)
Definition: def.c:90
netif
Definition: netif.h:260

Macro that generates the initial IP address to be tried by AUTOIP. If you want to override this, define it to something else in lwipopts.h.

## ◆ LWIP_AUTOIP_RAND

#define LWIP_AUTOIP_RAND | ( |  | netif | ) |

Value:
( (((u32_t)((netif->hwaddr[5]) & 0xff) << 24) | \
((u32_t)((netif->hwaddr[3]) & 0xff) << 16) | \
((u32_t)((netif->hwaddr[2]) & 0xff) << 8) | \
((u32_t)((netif->hwaddr[4]) & 0xff))) + \
(netif_autoip_data(netif)? netif_autoip_data(netif)->tried_llipaddr : 0))
netif::hwaddr
u8_t hwaddr[6U]
Definition: netif.h:341
netif
Definition: netif.h:260

Pseudo random macro based on netif informations. You could use "rand()" from the C Library if you define LWIP_AUTOIP_RAND in lwipopts.h

## Function Documentation

## ◆ autoip_arp_reply()

void autoip_arp_reply | ( | struct netif * | netif,
|  | struct etharp_hdr * | hdr
| ) |  |

Handles every incoming ARP Packet, called by etharp_input().

Parameters

  netif | network interface to use for autoip processing
  hdr | Incoming ARP packet

## ◆ autoip_network_changed()

void autoip_network_changed | ( | struct netif * | netif | ) |

Handle a possible change in the network configuration.

If there is an AutoIP address configured, take the interface down and begin probing with the same address.

## ◆ autoip_supplied_address()

u8_t autoip_supplied_address | ( | const struct netif * | netif | ) |

check if AutoIP supplied netif->ip_addr

Parameters

  netif | the netif to check

Returns
  1 if AutoIP supplied netif->ip_addr (state BOUND or ANNOUNCING), 0 otherwise

## ◆ autoip_tmr()

void autoip_tmr | ( | void |  | ) |

Has to be called in loop every AUTOIP_TMR_INTERVAL milliseconds