lwIP 2.1.0 Lightweight IP stack

Macros | Functions
icmp.c File Reference
`#include "lwip/opt.h"`
`#include "lwip/icmp.h"`
`#include "lwip/inet_chksum.h"`
`#include "lwip/ip.h"`
`#include "lwip/def.h"`
`#include "lwip/stats.h"`
`#include <string.h>`
`#include "path/to/my/lwip_hooks.h"`

## Macros
#define | LWIP_ICMP_ECHO_CHECK_INPUT_PBUF_LEN 1

## Functions
void | icmp_input (struct pbuf *p, struct netif *inp)
void | icmp_dest_unreach (struct pbuf *p, enum icmp_dur_type t)
void | icmp_time_exceeded (struct pbuf *p, enum icmp_te_type t)

## Detailed Description

ICMP - Internet Control Message Protocol

## Macro Definition Documentation

## ◆ LWIP_ICMP_ECHO_CHECK_INPUT_PBUF_LEN

#define LWIP_ICMP_ECHO_CHECK_INPUT_PBUF_LEN 1

Small optimization: set to 0 if incoming PBUF_POOL pbuf always can be used to modify and send a response packet (and to 1 if this is not the case, e.g. when link header is stripped off when receiving)

## Function Documentation

## ◆ icmp_dest_unreach()

void icmp_dest_unreach | ( | struct pbuf * | p,
|  | enum icmp_dur_type | t
| ) |  |

Send an icmp 'destination unreachable' packet, called from ip_input() if the transport layer protocol is unknown and from udp_input() if the local port is not bound.

Parameters

  p | the input packet for which the 'unreachable' should be sent, p->payload pointing to the IP header
  t | type of the 'unreachable' packet

## ◆ icmp_input()

void icmp_input | ( | struct pbuf * | p,
|  | struct netif * | inp
| ) |  |

Processes ICMP input packets, called from ip_input().

Currently only processes icmp echo requests and sends out the echo response.

Parameters

  p | the icmp echo request packet, p->payload pointing to the icmp header
  inp | the netif on which this packet was received

## ◆ icmp_time_exceeded()

void icmp_time_exceeded | ( | struct pbuf * | p,
|  | enum icmp_te_type | t
| ) |  |

Send a 'time exceeded' packet, called from ip_forward() if TTL is 0.

Parameters

  p | the input packet for which the 'time exceeded' should be sent, p->payload pointing to the IP header
  t | type of the 'time exceeded' packet