lwIP 2.1.1 Lightweight IP stack

Functions | Variables
timeouts.c File Reference
`#include "lwip/opt.h"`
`#include "lwip/timeouts.h"`
`#include "lwip/priv/tcp_priv.h"`
`#include "lwip/def.h"`
`#include "lwip/memp.h"`
`#include "lwip/priv/tcpip_priv.h"`
`#include "lwip/ip4_frag.h"`
`#include "lwip/etharp.h"`
`#include "lwip/dhcp.h"`
`#include "lwip/autoip.h"`
`#include "lwip/igmp.h"`
`#include "lwip/dns.h"`
`#include "lwip/nd6.h"`
`#include "lwip/ip6_frag.h"`
`#include "lwip/mld6.h"`
`#include "lwip/dhcp6.h"`
`#include "lwip/sys.h"`
`#include "lwip/pbuf.h"`

## Functions
void | tcp_timer_needed (void)
void | sys_timeouts_init (void)
void | sys_timeout (u32_t msecs, sys_timeout_handler handler, void *arg)
void | sys_untimeout (sys_timeout_handler handler, void *arg)
void | sys_check_timeouts (void)
void | sys_restart_timeouts (void)
u32_t | sys_timeouts_sleeptime (void)

## Variables
const struct lwip_cyclic_timer | lwip_cyclic_timers []
const int | lwip_num_cyclic_timers = (sizeof( lwip_cyclic_timers )/sizeof(( lwip_cyclic_timers )[0]))

## Detailed Description

Stack-internal timers implementation. This file includes timer callbacks for stack-internal timers as well as functions to set up or stop timers and check for expired timers.

## Function Documentation

## ◆ sys_restart_timeouts()

void sys_restart_timeouts | ( | void |  | ) |

Rebase the timeout times to the current time. This is necessary if sys_check_timeouts() hasn't been called for a long time (e.g. while saving energy) to prevent all timer functions of that period being called.

## ◆ sys_timeout()

void sys_timeout | ( | u32_t | msecs,
|  | sys_timeout_handler | handler,
|  | void * | arg
| ) |  |

Create a one-shot timer (aka timeout). Timeouts are processed in the following cases:

- while waiting for a message using sys_timeouts_mbox_fetch()
- by calling sys_check_timeouts() (NO_SYS==1 only)

Parameters

  msecs | time in milliseconds after that the timer should expire
  handler | callback function to call when msecs have elapsed
  arg | argument to pass to the callback function

## ◆ sys_timeouts_init()

void sys_timeouts_init | ( | void |  | ) |

Initialize this module

## ◆ sys_timeouts_sleeptime()

u32_t sys_timeouts_sleeptime | ( | void |  | ) |

Return the time left before the next timeout is due. If no timeouts are enqueued, returns 0xffffffff

## ◆ sys_untimeout()

void sys_untimeout | ( | sys_timeout_handler | handler,
|  | void * | arg
| ) |  |

Go through timeout list (for this task only) and remove the first matching entry (subsequent entries remain untouched), even though the timeout has not triggered yet.

Parameters

  handler | callback function that would be called by the timeout
  arg | callback argument that would be passed to handler

## ◆ tcp_timer_needed()

void tcp_timer_needed | ( | void |  | ) |

Called from TCP_REG when registering a new PCB: the reason is to have the TCP timer only running when there are active (or time-wait) PCBs.

## Variable Documentation

## ◆ lwip_cyclic_timers

const struct lwip_cyclic_timer lwip_cyclic_timers[]

This array contains all stack-internal cyclic timers. To get the number of timers, use LWIP_ARRAYSIZE()

## ◆ lwip_num_cyclic_timers

const int lwip_num_cyclic_timers = (sizeof( lwip_cyclic_timers )/sizeof(( lwip_cyclic_timers )[0]))

Array size of lwip_cyclic_timers[]