lwIP 2.1.1 Lightweight IP stack

Data Fields
netconn Struct Reference

`#include <api.h>`

## Data Fields
enum netconn_type | type
enum netconn_state | state
union {
} | pcb
err_t | pending_err
sys_sem_t | op_completed
sys_mbox_t | recvmbox
sys_mbox_t | acceptmbox
int | socket
s32_t | send_timeout
int | recv_bufsize
int | recv_avail
s16_t | linger
u8_t | flags
struct api_msg * | current_msg
netconn_callback | callback

## Detailed Description

A netconn descriptor

## Field Documentation

## ◆ acceptmbox

sys_mbox_t netconn::acceptmbox

mbox where new connections are stored until processed by the application thread

## ◆ callback

netconn_callback netconn::callback

A callback function that is informed about events for this netconn

## ◆ current_msg

struct api_msg* netconn::current_msg

TCP: when data passed to netconn_write doesn't fit into the send buffer, this temporarily stores the message. Also used during connect and close.

## ◆ flags

u8_t netconn::flags

flags holding more netconn-internal state, see NETCONN_FLAG_* defines

## ◆ linger

s16_t netconn::linger

values <0 mean linger is disabled, values > 0 are seconds to linger

## ◆ op_completed

sys_sem_t netconn::op_completed

sem that is used to synchronously execute functions in the core context

## ◆ pcb

union { ... } netconn::pcb

the lwIP internal protocol control block

## ◆ pending_err

err_t netconn::pending_err

the last asynchronous unreported error this netconn had

## ◆ recv_avail

int netconn::recv_avail

number of bytes currently in recvmbox to be received, tested against recv_bufsize to limit bytes on recvmbox for UDP and RAW, used for FIONREAD

## ◆ recv_bufsize

int netconn::recv_bufsize

maximum amount of bytes queued in recvmbox not used for TCP: adjust TCP_WND instead!

## ◆ recvmbox

sys_mbox_t netconn::recvmbox

mbox where received packets are stored until they are fetched by the netconn application thread (can grow quite big)

## ◆ send_timeout

s32_t netconn::send_timeout

timeout to wait for sending data (which means enqueueing data for sending in internal buffers) in milliseconds

## ◆ socket

int netconn::socket

only used for socket layer

## ◆ state

enum netconn_state netconn::state

current state of the netconn

## ◆ type

enum netconn_type netconn::type

type of the netconn (TCP, UDP or RAW)

The documentation for this struct was generated from the following file:

- src/include/lwip/api.h