lwIP 2.1.3 Lightweight IP stack

Data Fields
lwip_select_cb Struct Reference

`#include <sockets_priv.h>`

## Data Fields
struct lwip_select_cb * | next
struct lwip_select_cb * | prev
fd_set * | readset
fd_set * | writeset
fd_set * | exceptset
struct pollfd * | poll_fds
nfds_t | poll_nfds
int | sem_signalled
sys_sem_t | sem

## Detailed Description

Description for a task waiting in select

## Field Documentation

## ◆ exceptset

fd_set* lwip_select_cb::exceptset

unimplemented: exceptset passed to select

## ◆ next

struct lwip_select_cb* lwip_select_cb::next

Pointer to the next waiting task

## ◆ poll_fds

struct pollfd* lwip_select_cb::poll_fds

fds passed to poll; NULL if select

## ◆ poll_nfds

nfds_t lwip_select_cb::poll_nfds

nfds passed to poll; 0 if select

## ◆ prev

struct lwip_select_cb* lwip_select_cb::prev

Pointer to the previous waiting task

## ◆ readset

fd_set* lwip_select_cb::readset

readset passed to select

## ◆ sem

sys_sem_t lwip_select_cb::sem

semaphore to wake up a task waiting for select

## ◆ sem_signalled

int lwip_select_cb::sem_signalled

don't signal the same semaphore twice: set to 1 when signalled

## ◆ writeset

fd_set* lwip_select_cb::writeset

writeset passed to select

The documentation for this struct was generated from the following file:

- src/include/lwip/priv/sockets_priv.h