lwIP 2.1.3 Lightweight IP stack

Data Structures | Macros
etharp.h File Reference
`#include "lwip/arch.h"`
`#include "lwip/prot/ethernet.h"`
`#include "arch/bpstruct.h"`
`#include "arch/epstruct.h"`

## Data Structures
struct | ip4_addr_wordaligned
struct | etharp_hdr

## Macros
#define | IPADDR_WORDALIGNED_COPY_TO_IP4_ADDR_T(dest, src) SMEMCPY(dest, src, sizeof(ip4_addr_t))
#define | IPADDR_WORDALIGNED_COPY_FROM_IP4_ADDR_T(dest, src) SMEMCPY(dest, src, sizeof(ip4_addr_t))

## Detailed Description

ARP protocol definitions

## Macro Definition Documentation

## ◆ IPADDR_WORDALIGNED_COPY_FROM_IP4_ADDR_T

#define IPADDR_WORDALIGNED_COPY_FROM_IP4_ADDR_T | ( |  | dest,
|  |  | src
| ) |  | SMEMCPY(dest, src, sizeof(ip4_addr_t))

MEMCPY-like copying of IP addresses where addresses are known to be 16-bit-aligned if the port is correctly configured (so a port could define this to copying 2 u16_t's) - no NULL-pointer-checking needed.

## ◆ IPADDR_WORDALIGNED_COPY_TO_IP4_ADDR_T

#define IPADDR_WORDALIGNED_COPY_TO_IP4_ADDR_T | ( |  | dest,
|  |  | src
| ) |  | SMEMCPY(dest, src, sizeof(ip4_addr_t))

MEMCPY-like copying of IP addresses where addresses are known to be 16-bit-aligned if the port is correctly configured (so a port could define this to copying 2 u16_t's) - no NULL-pointer-checking needed.