# Release Notes

    Current Development
      - arduino package added
      - sniffer package added (moved from uracoli-appnotes)

    0.2.0  20120314
     New Features
      - generation of Makefile based source distribution
      - wireless bootloader (wibo) documented and added in
        source package
     New Hardware
      - Boards: stb128rfa1, muse231, zgbt1281a2uart0, zgbt1281a2uart1,
        zgbt1281a2nouart, im240a, im240a_eval, bitbean,
        cbb230[b], cbb231, cbb212, icm230_12a|b|c
     Changes/Misc
      - packages are now defined in packages.cfg instead in
        Tools/makerelease.sh
      - new example build scheme uses one (make,aps)-file per example.
      - software workaround for Sensor Terminal Board design issue, to
        avoid xmem bus contention
      - new documentaion scheme uses flat doxygen structure

    0.0.11 20100121
     New Features
      - added new hardware abstraction using board.cfg file
      - addded Zigbit Core for Arduino
      - added python serial throuput tool wuarttest.py
     New Hardware
      - MCU ATmega8, Atmega88, Atmega644P, ATmega128RFA1
      - Boards: littleGee V3, stkm8, rbb128rfa1, derfa1
     Bugs
      - #28148: incorporate patch that simplifies aps file generation
        (xsl transformation was replaced by simple text transformation)
     Changes/Misc
      - raven usb stick uses now correct uracoli VID/PID
      - clean up of warnings in the code
      - reworked linear buffer examples
      - refactoring of wuart application
      - io data handling in ieee802154_io.py
      - continued documentation

    0.0.10 20090721
      - added new buffer macros in ioutil.h
      - added FCTL macros in transceiver.h
      - updated examples for lgee and radio stream
        fixes in makerelease.sh

    0.0.9
      - no change tracking till here