Data Fields

# radio_param_t Union Reference
[Radio Access Functions]

Container for handover of radio parameter values. More...

## Data Fields
ccamode_t | cca_mode
channel_t | channel
uint8_t | data_rate
radio_state_t | idle_state
uint64_t * | long_addr
uint16_t | pan_id
uint16_t | short_addr
txpwr_t | tx_pwr

## Detailed Description

Container for handover of radio parameter values.

Note:
  The elements in this union should have max. a size of 2 byte, all other parameters should be configured with the void pointer.

## Field Documentation

ccamode_t radio_param_t::cca_mode

Value for cca mode.

channel_t radio_param_t::channel

Value for current radio channel. (MIN_CHANNEL ... MAX_CHANNEL)

uint8_t radio_param_t::data_rate

data rate type

radio_state_t radio_param_t::idle_state

after TX go to idle state

uint64_t* radio_param_t::long_addr

Pointer to long (64-bit) address

uint16_t radio_param_t::pan_id

Value for PANID

uint16_t radio_param_t::short_addr

Value for short address

txpwr_t radio_param_t::tx_pwr

Value for transmit power in dB.