# ioutil.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2007 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* The function keys_debounced() use the code given in Peter Fleury's
    00030    avr-gcc examples. File: avrgcc-examples/debounce_keys.c */
    00031
    00032 /****************************************************************************
    00033  Title:    Debouncing 8 Keys
    00034  Author:   Peter Fleury <pfleury@gmx.ch> http://jump.to/fleury,
    00035            based on algorithm of Peter Dannegger <danni@specs.de>
    00036  Date:     December 2003
    00037  Software: AVR-GCC 3.3
    00038  Hardware: AT90S8515 at 4 Mhz, STK200 compatible starter kit
    00039
    00040 *****************************************************************************/
    00041
    00042 /* $Id$ */
    00048 #ifndef IOUTIL_H
    00049 #define IOUTIL_H
    00050
    00051 /* === Includes ============================================================== */
    00052 #include <stdlib.h>
    00053 #include <stdio.h>
    00054 //#include <util/atomic.h>
    00055
    00056 #include "board.h"
    00057 #include "hif.h"
    00058 #include "timer.h"
    00059
    00060 /* === Externals ============================================================= */
    00061
    00062 /* === Types ================================================================= */
    00063
    00072 typedef struct
    00073 {
    00075     void * next;
    00077     uint8_t used;
    00079     uint8_t len;
    00081     uint8_t istart;
    00083     uint8_t iend;
    00085     uint8_t data[];
    00086 } buffer_t;
    00087
    00088
    00089 typedef struct
    00090 {
    00092     uint8_t nb;
    00094     uint8_t elsz;
    00096     uint8_t pool[];
    00097 } buffer_pool_t;
    00098
    00101 /* === Macros ================================================================ */
    00102
    00103 /* === LED Handling === */
    00104
    00108 #if defined(NO_LEDS) || defined (DOXYGEN)
    00109 # undef LED_NUMBER
    00110
    00111 # define LED_NUMBER    (0)
    00112 #endif
    00113
    00114 #if defined(NO_LEDS) || defined (DOXYGEN)
    00115
    00116 # define LED_INIT() do{}while(0)
    00117 #elif !defined(LED_INIT)
    00118 # if LEDS_INVERSE == 0
    00119 #  define LED_INIT() LED_DDR |= (LED_MASK); LED_PORT &= ~(LED_MASK)
    00120 # else
    00121 #   define LED_INIT() LED_DDR |= (LED_MASK); LED_PORT |= (LED_MASK)
    00122 # endif
    00123 #endif /* !defined(LED_INIT)*/
    00124
    00125 #if defined(NO_LEDS) || defined (DOXYGEN)
    00126
    00131 # define LED_SET_VALUE(x) do{}while(0)
    00132 #elif !defined(LED_SET_VALUE)
    00133 # if LEDS_INVERSE == 0
    00134 #  define LED_SET_VALUE(x) \
    00135             do {\
    00136                 LED_PORT = (LED_PORT & ~LED_MASK) | ((x<<LED_SHIFT) & LED_MASK);\
    00137             }while(0)
    00138 # else
    00139 #  define LED_SET_VALUE(x) do {\
    00140             LED_PORT = (LED_PORT & ~LED_MASK) | ((~x<<LED_SHIFT) & LED_MASK);\
    00141             }while(0)
    00142 # endif
    00143 #endif /* !defined(LED_SET_VALUE)*/
    00144
    00145 #if defined(NO_LEDS) || defined (DOXYGEN)
    00146
    00147 # define LED_GET_VALUE() 0
    00148 #elif !defined(LED_GET_VALUE)
    00149 # if LEDS_INVERSE == 0
    00150 #  define LED_GET_VALUE()  ((LED_PORT & LED_MASK) >> LED_SHIFT)
    00151 # else
    00152 #  define LED_GET_VALUE()  ((~LED_PORT & LED_MASK) >> LED_SHIFT)
    00153 # endif
    00154 #endif /* !defined(LED_GET_VALUE)*/
    00155
    00156
    00157 #if defined(NO_LEDS) || defined (DOXYGEN)
    00158
    00159 # define LED_SET(ln) do{}while(0)
    00160 #elif !defined(LED_SET)
    00161 # if LEDS_INVERSE == 0
    00162 #  define LED_SET(ln)      LED_PORT |= (_BV(ln+LED_SHIFT) & LED_MASK)
    00163 # else
    00164 #  define LED_SET(ln)      LED_PORT &= ~(_BV(ln+LED_SHIFT) & LED_MASK)
    00165 # endif
    00166 #endif /* !defined(LED_SET)*/
    00167
    00168
    00169 #if defined(NO_LEDS) || defined (DOXYGEN)
    00170
    00171 # define LED_CLR(ln) do{}while(0)
    00172 #elif !defined(LED_CLR)
    00173 # if LEDS_INVERSE == 0
    00174 #  define LED_CLR(ln)      LED_PORT &= ~(_BV(ln+LED_SHIFT) & LED_MASK)
    00175 # else
    00176 #  define LED_CLR(ln)      LED_PORT |= (_BV(ln+LED_SHIFT) & LED_MASK)
    00177 # endif
    00178 #endif /* !defined(LED_CLR)*/
    00179
    00180 #if defined(NO_LEDS) || defined (DOXYGEN)
    00181
    00182 # define LED_VAL(msk,val) do{}while(0)
    00183 #elif !defined(LED_VAL)
    00184 # if LEDS_INVERSE == 0
    00185 #  define LED_VAL(msk,val) LED_PORT |= ((LED_MASK|msk) << LED_SHIFT); \
    00186                            LED_PORT |= ~((val << LED_SHIFT)& (LED_MASK|(msk<<LED_SHIFT)) )
    00187 # else
    00188 #  define LED_VAL(msk,val) LED_PORT &= ~(LED_MASK|(msk<<LED_SHIFT)); LED_PORT |= ~(val & (LED_MASK|msk))
    00189
    00190 # endif
    00191 #endif /* !defined(LED_VAL)*/
    00192
    00193 #if defined(NO_LEDS) || defined (DOXYGEN)
    00194
    00195 # define LED_TOGGLE(ln) do{}while(0)
    00196 #elif !defined(LED_TOGGLE)
    00197 # define LED_TOGGLE(ln) LED_PORT ^= (_BV(ln+LED_SHIFT) & LED_MASK)
    00198 #endif /* !defined(LED_TOGGLE)*/
    00199
    00201 #define LED_MAX_VALUE ((1<<LED_NUMBER)-1)
    00202
    00206 /* === KEY Handling === */
    00207
    00212 #if defined(NO_KEYS) || defined (DOXYGEN)
    00213
    00214 # define KEY_INIT()
    00215
    00217 # define KEY_GET() (0)
    00218
    00219 #else /* defined(NO_KEYS) || defined (DOXYGEN) */
    00220 # if PULLUP_KEYS != 0
    00221 #  define PULL_MASK (MASK_KEY)
    00222 # else /* PULLUP_KEYS != 0 */
    00223 #  define PULL_MASK (0)
    00224 # endif /* PULLUP_KEYS != 0 */
    00225 # if !defined KEY_INIT
    00226 #  define KEY_INIT()  do{PORT_KEY |= PULL_MASK; DDR_KEY &= ~(MASK_KEY); }while(0)
    00227 # endif
    00228 # if !defined KEY_GET
    00229 # if INVERSE_KEYS == 0
    00230 #  define KEY_GET()\
    00231                 ((PIN_KEY & MASK_KEY) >> SHIFT_KEY)
    00232 # else /* INVERSE_KEYS == 0 */
    00233 #  define KEY_GET()\
    00234                 ((~PIN_KEY & MASK_KEY) >> SHIFT_KEY)
    00235 # endif /* INVERSE_KEYS == 0 */
    00236 # endif /* !defined KEY_GET */
    00237 #endif /* defined(NO_KEYS) || defined (DOXYGEN) */
    00238
    00239
    00240
    00245 static inline uint8_t keys_debounced(void)
    00246 {
    00247   static uint8_t key_state;     // debounced and inverted key state:
    00248   static uint8_t ct0, ct1;      // holds two bit counter for each key
    00249   uint8_t i;
    00250
    00251
    00252   /*
    00253    * read current state of keys (active-low),
    00254    * clear corresponding bit in i when key has changed
    00255    */
    00256   i = key_state ^ KEY_GET();   // key changed ?
    00257
    00258   /*
    00259    * ct0 and ct1 form a two bit counter for each key,
    00260    * where ct0 holds LSB and ct1 holds MSB
    00261    * After a key is pressed longer than four times the
    00262    * sampling period, the corresponding bit in key_state is set
    00263    */
    00264   ct0 = ~( ct0 & i );           // reset or count ct0
    00265   ct1 = (ct0 ^ ct1) & i;        // reset or count ct1
    00266   i &= ct0 & ct1;               // count until roll over ?
    00267   key_state ^= i;               // then toggle debounced state
    00268
    00269   /*
    00270    * To notify main program of pressed key, the correspondig bit
    00271    * in global variable key_press is set.
    00272    * The main loop needs to clear this bit
    00273    */
    00274   return key_state & i; // 0->1: key press detect
    00275
    00276 }
    00277
    00282 static inline void trap_if_key_pressed(void)
    00283 {
    00284
    00285     KEY_INIT();
    00286     DELAY_MS(10);
    00287     if (KEY_GET())
    00288     {
    00289         LED_INIT();
    00290         while(1)
    00291         {
    00292             DELAY_MS(400);
    00293             LED_SET(0);
    00294             DELAY_MS(10);
    00295             LED_CLR(0);
    00296         }
    00297     }
    00298 }
    00299
    00302 /* === Bootloader Interface === */
    00303 #if BOOT_LOADER_ADDRESS != 0
    00304
    00305 #define JUMP_BOOT_LOADER() \
    00306     do {\
    00307         void (*funcptr)( uint8_t flag ) = BOOT_LOADER_ADDRESS;\
    00308         funcptr(42);\
    00309     }while(0)
    00310 #else /* BOOT_LOADER_ADDRESS != 0 */
    00311 #define JUMP_BOOT_LOADER()
    00312 #endif /* BOOT_LOADER_ADDRESS != 0 */
    00313
    00314
    00315
    00316
    00317 /* === Prototypes ============================================================ */
    00318 #ifdef __cplusplus
    00319 extern "C" {
    00320 #endif
    00321
    00325 #if 0
    00326 #define BUFFER_SET_USED(b) do{ATOMIC_BLOCK(ATOMIC_FORCEON){b->used|=1}}while(0)
    00327 #define BUFFER_SET_UNUSED(b) do{ATOMIC_BLOCK(ATOMIC_FORCEON){b->used&=~1}}while(0)
    00328 #define BUFFER_IS_USED(b) ((b->used&1)!=0)
    00329
    00330 #define BUFFER_SET_LOCK(b) do{ATOMIC_BLOCK(ATOMIC_FORCEON){b->used|=2}}while(0)
    00331 #define BUFFER_SET_UNLOCK(b) do{ATOMIC_BLOCK(ATOMIC_FORCEON){b->used&=~2}}while(0)
    00332 #define BUFFER_IS_LOCKED(b) ((b->used&2)!=0)
    00333 #endif
    00334
    00335 #define BUFFER_SET_USED(b) do{b->used|=1;}while(0)
    00336 #define BUFFER_SET_UNUSED(b) do{b->used&=~1;}while(0)
    00337 #define BUFFER_IS_USED(b) ((b->used&1)!=0)
    00338
    00339 #define BUFFER_SET_LOCK(b) do{b->used|=2;}while(0)
    00340 #define BUFFER_SET_UNLOCK(b) do{b->used&=~2;}while(0)
    00341 #define BUFFER_IS_LOCKED(b) ((b->used&2)!=0)
    00342
    00343
    00344 #define BUFFER_SIZE(b) (b->iend - b->istart)
    00345 #define BUFFER_PDATA(b) (b->data + b->istart)
    00346 #define BUFFER_SEEK(b,offset) (b->data + (b->iend=offset))
    00347
    00348 #define BUFFER_GET_MEMBLOCK(b,pmem,size) \
    00349     do{\
    00350         b->used = 1;\
    00351         pmem = (b->data + b->iend);\
    00352         size = (b->len - b->iend);\
    00353     }while(0)
    00354
    00355 #define BUFFER_UPDATE_MEMBLOCK(b,end) \
    00356     do{\
    00357         b->iend = end;\
    00358         b->used = 0;\
    00359     }while(0);
    00360
    00361 #define BUFFER_LAST_CHAR(b) \
    00362     (b->iend <= b->istart) ? EOF : (char)b->data[b->iend-1]
    00363 #define BUFFER_FREE_AT_END(b) (b->len - b->iend)
    00364 #define BUFFER_FREE_AT_START(b) (b->istart)
    00365 #define BUFFER_ELSZ(x) (sizeof(buffer_t) + (x))
    00366 #define BUFFER_RESET(b,start) do{ b->iend = b->istart = start;}while(0)
    00367 #define BUFFER_ADVANCE(b,more) do{ b->istart += more;}while(0)
    00368
    00370 buffer_t * buffer_init(void * pmem, uint8_t size, uint8_t start);
    00372 int buffer_append_char(buffer_t *b, uint8_t c);
    00374 int buffer_prepend_char(buffer_t *b, int c);
    00376 int buffer_get_char(buffer_t *b);
    00378 uint8_t buffer_append_block(buffer_t *b, void *pdata, uint8_t size);
    00380 uint8_t buffer_prepend_block(buffer_t *b, void *pdata, uint8_t size);
    00382 uint8_t buffer_get_block(buffer_t *b, void *pdata, uint8_t size);
    00383
    00384
    00385 buffer_pool_t * buffer_pool_init(uint8_t *pmem, size_t memsz, uint8_t bsz);
    00386 buffer_t * buffer_alloc(buffer_pool_t *ppool, uint8_t istart);
    00387 void buffer_free(buffer_t * pbuf);
    00388
    00389
    00390
    00391 /* buffer stream function */
    00392 //typedef void (*incb)(buffer_t *pbuf) buffer_stream_incb_t;
    00393 //typedef void (*outcb)(buffer_t *pbuf) buffer_stream_outcb_t;
    00394
    00395 typedef struct
    00396 {
    00397     FILE bstream;
    00398     buffer_t *pbufin;
    00399     buffer_t *pbufout;
    00400     void (*incb)(buffer_t *pbuf);
    00401     void (*outcb)(buffer_t *pbuf);
    00402 } buffer_stream_t;
    00403
    00404
    00405
    00406 int buffer_stream_init( buffer_stream_t *pbs,
    00407                         void (*incb)(buffer_t *pbuf),
    00408                         void (*outcb)(buffer_t *pbuf));
    00409
    00410 int buffer_stream_putchar(char c,FILE *f);
    00411 int buffer_stream_getchar(FILE *f);
    00412
    00413
    00414
    00416 #ifdef __cplusplus
    00417 } /* extern "C" */
    00418 #endif
    00419
    00420 #endif  /* #ifndef IOUTIL_H */
    00421 /* EOF */