# Using USB connected Programmers under Linux

SuSE 11.0

     cd  /etc/udev/rules.d/80-usbprog.rules
     vi 80-usbprog.rules

In this file add the following lines:

     # AVR ISP
     ATTR{idVendor}=="03eb", ATTR{idProduct}=="2104", GROUP="users", MODE="0660"
     # AVR Dragon
     ATTR{idVendor}=="03eb", ATTR{idProduct}=="2107", GROUP="users", MODE="0660"
     # JTAG ICE MkII
     ATTR{idVendor}=="03eb", ATTR{idProduct}=="2103", GROUP="users", MODE="0660"

If you want to enable other USB devices for users access, just check the output of lsusb command.

     $$ lsusb
      ...
      Bus 006 Device 001: ID 1d6b:0001 Linux Foundation 1.1 root hub
      Bus 002 Device 009: ID 03eb:2103 Atmel Corp. JTAG ICE mkII
      Bus 002 Device 003: ID 07d1:3c03 D-Link System DWL-G122 802.11g Adapter [ralink rt73]
      Bus 002 Device 002: ID 0409:005a NEC Corp. HighSpeed Hub
      ...

Thanks to the german description at: http://www.wiki.elektronik-projekt.de/mikrocontroller/avr/avrdude

SuSE 10.0

Add the following line at the end of file /etc/udev/rules.d/50-udev.rules

     SUBSYSTEM=="usb", ACTION=="add", ENV{PRODUCT}=="3eb/2103/*", RUN+="/bin/sh -c '/bin/chgrp uucp $env{DEVICE} ; /bin/chmod g+w $env{DEVICE}'"