# xmpl_key_events.c - Implementing Key Events

## Key Event Example

    /* $Id$ */
    /* Example for key event processing with a single  key */

    #include "ioutil.h"
    #include "timer.h"
    #include "xmpl.h"

    #define SHORT_PRESS_TICKS  (MSEC(100))
    #define MEDIUM_PRESS_TICKS (MSEC(300))
    #define LONG_PRESS_TICKS   (MSEC(800))

    #define NONE_PRESS   (0)
    #define SHORT_PRESS  (1)
    #define MEDIUM_PRESS (2)
    #define LONG_PRESS   (3)
    #define CONT_PRESS   (4)

    volatile uint8_t KeyEvent = 0;

    static uint8_t debounce_key0(void)
    {
    uint8_t ret, tmp;
    static uint16_t ocnt=0, ccnt=0;

        ret = NONE_PRESS;
        tmp = (KEY_GET() & 1);
        if (tmp != 0)
        {
            ocnt ++;
            if(ocnt >= LONG_PRESS_TICKS)
            {
                ocnt = LONG_PRESS_TICKS;
                ccnt++;
                if (ccnt >= MEDIUM_PRESS_TICKS)
                {
                    ccnt = 0;
                    ret = CONT_PRESS;
                }
            }
        }
        else
        {
            if(ocnt >= LONG_PRESS_TICKS)
            {
                ret = LONG_PRESS;
            }
            else if(ocnt >= MEDIUM_PRESS_TICKS)
            {
                ret = MEDIUM_PRESS;
            }
            else if(ocnt >= SHORT_PRESS_TICKS)
            {
                ret = SHORT_PRESS;
            }
            ccnt = 0;
            ocnt = 0;
        }

        return ret;
    }

    int main(void)
    {
        uint8_t tmp;

        KEY_INIT();
        LED_INIT();
        TIMER_INIT();
        sei();
        while(1)
        {
            if (KeyEvent == SHORT_PRESS)
            {
                LED_TOGGLE(0);
            }

            if (KeyEvent == MEDIUM_PRESS)
            {
                LED_TOGGLE(1);
            }

            if (KeyEvent == LONG_PRESS)
            {
                LED_SET_VALUE(0);
            }
            if (KeyEvent == CONT_PRESS)
            {
                tmp = LED_GET_VALUE();
                tmp ++;
                LED_SET_VALUE(tmp);
            }
            KeyEvent = NONE_PRESS;
            SLEEP_ON_IDLE();
        }
    }

    ISR(TIMER_IRQ_vect)
    {
        if (KeyEvent == NONE_PRESS)
        {
            KeyEvent = debounce_key0();
        }
    }
    /* EOF */