Data Fields

# radio_status_t Struct Reference
[Radio Access Functions]

Structure for storage of radio parameters. More...

## Data Fields
uint8_t | cca_mode
uint8_t | channel
radio_state_t | idle_state
uint8_t * | rxframe
uint8_t | rxframesz
radio_state_t | state
uint8_t | tx_pwr

## Detailed Description

Structure for storage of radio parameters.

## Field Documentation

uint8_t radio_status_t::cca_mode

Current cca mode.

uint8_t radio_status_t::channel

Current radio channel. (MIN_CHANNEL ... MAX_CHANNEL)

radio_state_t radio_status_t::idle_state

after TX go to idle state

uint8_t* radio_status_t::rxframe

Pointer for frame data storage.

uint8_t radio_status_t::rxframesz

Length of the buffer rxframesz

radio_state_t radio_status_t::state

Current transceiver state.

uint8_t radio_status_t::tx_pwr

Current transmit power.