# at86rf212.h

Go to the documentation of this file.

    00001 /* THIS FILE IS GENERATED by ds2reg.py FROM INPUT Templates/at86rf212.txt */
    00002
    00003 /* Copyright (c) 2008 Axel Wachtler
    00004    All rights reserved.
    00005
    00006    Redistribution and use in source and binary forms, with or without
    00007    modification, are permitted provided that the following conditions
    00008    are met:
    00009
    00010    * Redistributions of source code must retain the above copyright
    00011      notice, this list of conditions and the following disclaimer.
    00012    * Redistributions in binary form must reproduce the above copyright
    00013      notice, this list of conditions and the following disclaimer in the
    00014      documentation and/or other materials provided with the distribution.
    00015    * Neither the name of the authors nor the names of its contributors
    00016      may be used to endorse or promote products derived from this software
    00017      without specific prior written permission.
    00018
    00019    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00020    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00021    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00022    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00023    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00024    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00025    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00026    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00027    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00028    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00029    POSSIBILITY OF SUCH DAMAGE. */
    00030
    00031 /* $Id$ */
    00036 #ifndef AT86RF212_H
    00037 #define AT86RF212_H (1)
    00038 /* === Includes ============================================================== */
    00039
    00040 /* === Externals ============================================================= */
    00041
    00042 /* === Types ================================================================= */
    00043
    00044 typedef uint8_t trx_ramaddr_t;
    00045 typedef uint8_t trx_regval_t;
    00046 typedef uint8_t trx_regaddr_t;
    00047
    00048 /* === Macros ================================================================ */
    00050 #define RG_TRX_STATUS (0x1)
    00051
    00052   #define SR_CCA_DONE 0x1,0x80,7
    00053
    00054   #define SR_CCA_STATUS 0x1,0x40,6
    00055
    00056   #define SR_TRX_STATUS 0x1,0x1f,0
    00057     #define P_ON (0)
    00058     #define BUSY_RX (1)
    00059     #define BUSY_TX (2)
    00060     #define RX_ON (6)
    00061     #define TRX_OFF (8)
    00062     #define PLL_ON (9)
    00063     #define TRX_SLEEP (15)
    00064     #define BUSY_RX_AACK (17)
    00065     #define BUSY_TX_ARET (18)
    00066     #define RX_AACK_ON (22)
    00067     #define TX_ARET_ON (25)
    00068     #define RX_ON_NOCLK (28)
    00069     #define RX_AACK_ON_NOCLK (29)
    00070     #define BUSY_RX_AACK_NOCLK (30)
    00071
    00072 #define RG_TRX_STATE (0x2)
    00073
    00074   #define SR_TRAC_STATUS 0x2,0xe0,5
    00075     #define TRAC_SUCCESS (0)
    00076     #define TRAC_SUCCESS_DATA_PENDING (1)
    00077     #define TRAC_SUCCESS_WAIT_FOR_ACK (2)
    00078     #define TRAC_CHANNEL_ACCESS_FAILURE (3)
    00079     #define TRAC_NO_ACK (5)
    00080     #define TRAC_INVALID (7)
    00081
    00082   #define SR_TRX_CMD 0x2,0x1f,0
    00083     #define CMD_NOP (0)
    00084     #define CMD_TX_START (2)
    00085     #define CMD_FORCE_TRX_OFF (3)
    00086     #define CMD_RX_ON (6)
    00087     #define CMD_TRX_OFF (8)
    00088     #define CMD_PLL_ON (9)
    00089     #define CMD_RX_AACK_ON (22)
    00090     #define CMD_TX_ARET_ON (25)
    00091
    00092 #define RG_TRX_CTRL_0 (0x3)
    00093
    00094   #define SR_PAD_IO 0x3,0xc0,6
    00095
    00096   #define SR_PAD_IO_CLKM 0x3,0x30,4
    00097     #define CLKM_2mA (0)
    00098     #define CLKM_4mA (1)
    00099     #define CLKM_6mA (2)
    00100     #define CLKM_8mA (3)
    00101
    00102   #define SR_CLKM_SHA_SEL 0x3,0x8,3
    00103
    00104   #define SR_CLKM_CTRL 0x3,0x7,0
    00105     #define CLKM_no_clock (0)
    00106     #define CLKM_1MHz (1)
    00107     #define CLKM_2MHz (2)
    00108     #define CLKM_4MHz (3)
    00109     #define CLKM_8MHz (4)
    00110     #define CLKM_16MHz (5)
    00111
    00112 #define RG_TRX_CTRL_1 (0x4)
    00113
    00114   #define SR_PA_EXT_EN 0x4,0x80,7
    00115
    00116   #define SR_IRQ_2_EXT_EN 0x4,0x40,6
    00117
    00118   #define SR_TX_AUTO_CRC_ON 0x4,0x20,5
    00119
    00120   #define SR_RX_BL_CTRL 0x4,0x10,4
    00121
    00122   #define SR_SPI_CMD_MODE 0x4,0xc,2
    00123
    00124   #define SR_IRQ_POLARITY 0x4,0x1,0
    00125
    00126   #define SR_IRQ_MASK_MODE 0x4,0x2,1
    00127
    00128 #define RG_PHY_TX_PWR (0x5)
    00129
    00130   #define SR_PA_BOOST 0x5,0x80,7
    00131
    00132   #define SR_GC_PA 0x5,0x60,5
    00133
    00134   #define SR_TX_PWR 0x5,0x1f,0
    00135
    00136 #define RG_PHY_RSSI (0x6)
    00137
    00138   #define SR_RX_CRC_VALID 0x6,0x80,7
    00139
    00140   #define SR_RND_VALUE 0x6,0x60,5
    00141
    00142   #define SR_RSSI 0x6,0x1f,0
    00143
    00144 #define RG_PHY_ED_LEVEL (0x7)
    00145
    00146   #define SR_ED_LEVEL 0x7,0xff,0
    00147
    00148 #define RG_PHY_CC_CCA (0x8)
    00149
    00150   #define SR_CCA_REQUEST 0x8,0x80,7
    00151
    00152   #define SR_CCA_MODE 0x8,0x60,5
    00153
    00154   #define SR_CHANNEL 0x8,0x1f,0
    00155
    00156 #define RG_CCA_THRES (0x9)
    00157
    00158   #define SR_CCA_ED_THRES 0x9,0xf,0
    00159
    00160 #define RG_SFD_VALUE (0xb)
    00161
    00162   #define SR_SFD_VALUE 0xb,0xff,0
    00163
    00164 #define RG_TRX_CTRL_2 (0xc)
    00165
    00166   #define SR_RX_SAFE_MODE 0xc,0x80,7
    00167
    00168   #define SR_TRX_OFF_AVDD_EN 0xc,0x40,6
    00169
    00170   #define SR_BPSK_OQPSK 0xc,0x8,3
    00171
    00172   #define SR_SUB_MODE 0xc,0x4,2
    00173
    00174   #define SR_OQPSK_DATA_RATE 0xc,0x3,0
    00175
    00176 #define RG_ANT_DIV (0xd)
    00177
    00178   #define SR_ANT_SEL 0xd,0x80,7
    00179
    00180   #define SR_ANT_EXT_SW_EN 0xd,0x4,2
    00181
    00182   #define SR_ANT_CTRL 0xd,0x3,0
    00183
    00184 #define RG_IRQ_MASK (0xe)
    00185
    00186   #define SR_MASK_BAT_LOW 0xe,0x80,7
    00187
    00188   #define SR_MASK_TRX_UR 0xe,0x40,6
    00189
    00190   #define SR_MASK_AMI 0xe,0x20,5
    00191
    00192   #define SR_MASK_CCA_ED_READY 0xe,0x10,4
    00193
    00194   #define SR_MASK_TRX_END 0xe,0x8,3
    00195
    00196   #define SR_MASK_RX_START 0xe,0x4,2
    00197
    00198   #define SR_MASK_PLL_LOCK 0xe,0x1,0
    00199
    00200   #define SR_MASK_PLL_UNLOCK 0xe,0x2,1
    00201
    00202 #define RG_IRQ_STATUS (0xf)
    00203
    00204   #define SR_BAT_LOW 0xf,0x80,7
    00205
    00206   #define SR_TRX_UR 0xf,0x40,6
    00207
    00208   #define SR_AMI 0xf,0x20,5
    00209
    00210   #define SR_CCA_ED_READY 0xf,0x10,4
    00211
    00212   #define SR_TRX_END 0xf,0x8,3
    00213
    00214   #define SR_RX_START 0xf,0x4,2
    00215
    00216   #define SR_PLL_LOCK 0xf,0x1,0
    00217
    00218   #define SR_PLL_UNLOCK 0xf,0x2,1
    00219
    00220 #define RG_VREG_CTRL (0x10)
    00221
    00222   #define SR_AVREG_EXT 0x10,0x80,7
    00223
    00224   #define SR_AVDD_OK 0x10,0x40,6
    00225
    00226   #define SR_DVREG_EXT 0x10,0x8,3
    00227
    00228   #define SR_DVDD_OK 0x10,0x4,2
    00229
    00230 #define RG_BATMON (0x11)
    00231
    00232   #define SR_BATMON_OK 0x11,0x20,5
    00233
    00234   #define SR_BATMON_HR 0x11,0x10,4
    00235
    00236   #define SR_BATMON_VTH 0x11,0xf,0
    00237
    00238 #define RG_XOSC_CTRL (0x12)
    00239
    00240   #define SR_XTAL_MODE 0x12,0xf0,4
    00241
    00242   #define SR_XTAL_TRIM 0x12,0xf,0
    00243
    00244 #define RG_CC_CTRL_0 (0x13)
    00245
    00246   #define SR_CC_NUMBER 0x13,0xff,0
    00247
    00248 #define RG_CC_CTRL_1 (0x14)
    00249
    00250   #define SR_CC_BAND 0x14,0x4,2
    00251
    00252   #define SR_BAND 0x14,0x1,0
    00253
    00254   #define SR_CC_ 0x14,0x2,1
    00255
    00256 #define RG_RX_SYN (0x15)
    00257
    00258   #define SR_RX_PDT_DIS 0x15,0x80,7
    00259
    00260   #define SR_RX_PDT_LEVEL 0x15,0xf,0
    00261
    00262 #define RG_RF_CTRL_0 (0x16)
    00263
    00264   #define SR_PA_LT 0x16,0xc0,6
    00265
    00266   #define SR_GC_TX_OFFS 0x16,0x3,0
    00267
    00268 #define RG_XAH_CTRL_1 (0x17)
    00269
    00270   #define SR_CSMA_LBT_MODE 0x17,0x80,7
    00271
    00272   #define SR_AACK_FLTR_RES_FT 0x17,0x20,5
    00273
    00274   #define SR_AACK_UPLD_RES_FT 0x17,0x10,4
    00275
    00276   #define SR_AACK_ACK_TIME 0x17,0x4,2
    00277
    00278   #define SR_AACK_PROM_MODE 0x17,0x2,1
    00279
    00280 #define RG_FTN_CTRL (0x18)
    00281
    00282   #define SR_FTN_START 0x18,0x80,7
    00283
    00284 #define RG_RF_CTRL_1 (0x19)
    00285
    00286   #define SR_RF_MC 0x19,0xf0,4
    00287
    00288 #define RG_PLL_CF (0x1a)
    00289
    00290   #define SR_PLL_CF_START 0x1a,0x80,7
    00291
    00292 #define RG_PLL_DCU (0x1b)
    00293
    00294   #define SR_PLL_DCU_START 0x1b,0x80,7
    00295
    00296 #define RG_PART_NUM (0x1c)
    00297
    00298   #define SR_PART_NUM 0x1c,0xff,0
    00299     #define RF212A_PART_NUM (7)
    00300
    00301 #define RG_VERSION_NUM (0x1d)
    00302
    00303   #define SR_VERSION_NUM 0x1d,0xff,0
    00304     #define RF212A_VERSION_NUM (1)
    00305
    00306 #define RG_MAN_ID_0 (0x1e)
    00307
    00308   #define SR_MAN_ID_0 0x1e,0xff,0
    00309
    00310 #define RG_MAN_ID_1 (0x1f)
    00311
    00312   #define SR_MAN_ID_1 0x1f,0xff,0
    00313
    00314 #define RG_SHORT_ADDR_0 (0x20)
    00315
    00316   #define SR_SHORT_ADDR_0 0x20,0xff,0
    00317
    00318 #define RG_SHORT_ADDR_1 (0x21)
    00319
    00320   #define SR_SHORT_ADDR_1 0x21,0xff,0
    00321
    00322 #define RG_PAN_ID_0 (0x22)
    00323
    00324   #define SR_PAN_ID_0 0x22,0xff,0
    00325
    00326 #define RG_PAN_ID_1 (0x23)
    00327
    00328   #define SR_PAN_ID_1 0x23,0xff,0
    00329
    00330 #define RG_IEEE_ADDR_0 (0x24)
    00331
    00332   #define SR_IEEE_ADDR_0 0x24,0xff,0
    00333
    00334 #define RG_IEEE_ADDR_1 (0x25)
    00335
    00336   #define SR_IEEE_ADDR_1 0x25,0xff,0
    00337
    00338 #define RG_IEEE_ADDR_2 (0x26)
    00339
    00340   #define SR_IEEE_ADDR_2 0x26,0xff,0
    00341
    00342 #define RG_IEEE_ADDR_3 (0x27)
    00343
    00344   #define SR_IEEE_ADDR_3 0x27,0xff,0
    00345
    00346 #define RG_IEEE_ADDR_4 (0x28)
    00347
    00348   #define SR_IEEE_ADDR_4 0x28,0xff,0
    00349
    00350 #define RG_IEEE_ADDR_5 (0x29)
    00351
    00352   #define SR_IEEE_ADDR_5 0x29,0xff,0
    00353
    00354 #define RG_IEEE_ADDR_6 (0x2a)
    00355
    00356   #define SR_IEEE_ADDR_6 0x2a,0xff,0
    00357
    00358 #define RG_IEEE_ADDR_7 (0x2b)
    00359
    00360   #define SR_IEEE_ADDR_7 0x2b,0xff,0
    00361
    00362 #define RG_XAH_CTRL_0 (0x2c)
    00363
    00364   #define SR_MAX_FRAME_RETRIES 0x2c,0xf0,4
    00365
    00366   #define SR_SLOTTED_OPERATION 0x2c,0x1,0
    00367
    00368   #define SR_MAX_CSMA_RETRIES 0x2c,0xe,1
    00369
    00370 #define RG_CSMA_SEED_0 (0x2d)
    00371
    00372   #define SR_CSMA_SEED_0 0x2d,0xff,0
    00373
    00374 #define RG_CSMA_SEED_1 (0x2e)
    00375
    00376   #define SR_AACK_FVN_MODE 0x2e,0xc0,6
    00377
    00378   #define SR_AACK_SET_PD 0x2e,0x20,5
    00379
    00380   #define SR_AACK_DIS_ACK 0x2e,0x10,4
    00381
    00382   #define SR_AACK_I_AM_COORD 0x2e,0x8,3
    00383
    00384   #define SR_CSMA_SEED_1 0x2e,0x7,0
    00385
    00386 #define RG_CSMA_BE (0x2f)
    00387
    00388   #define SR_MAX_BE 0x2f,0xf0,4
    00389
    00390   #define SR_MIN_BE 0x2f,0xf,0
    00391
    00392 #define RADIO_NAME "AT86RF212"
    00393
    00394 #define RADIO_PART_NUM (RF212A_PART_NUM)
    00395
    00396 #define RADIO_VERSION_NUM (RF212A_VERSION_NUM)
    00397
    00399 #define TRX_CMD_RW           (_BV(7) | _BV(6))
    00400
    00401 #define TRX_CMD_RR           (_BV(7))
    00402
    00403 #define TRX_CMD_FW           (_BV(6) | _BV(5))
    00404
    00405 #define TRX_CMD_FR           (_BV(5))
    00406
    00407 #define TRX_CMD_SW           (_BV(6))
    00408
    00409 #define TRX_CMD_SR           (0)
    00410
    00411 #define TRX_CMD_RADDR_MASK   (0x3f)
    00412
    00414 #define TRX_RESET_TIME_US    (6)
    00415
    00417 #define TRX_INIT_TIME_US     (510)
    00418
    00420 #define TRX_PLL_LOCK_TIME_US     (180)
    00421
    00422
    00424 #define TRX_CCA_TIME_US     (140)
    00425
    00427 #define TRX_IRQ_PLL_LOCK   _BV(0)
    00428
    00430 #define TRX_IRQ_PLL_UNLOCK _BV(1)
    00431
    00433 #define TRX_IRQ_RX_START   _BV(2)
    00434
    00436 #define TRX_IRQ_TRX_END    _BV(3)
    00437
    00439 #define TRX_IRQ_CCA_ED     _BV(4)
    00440
    00442 #define TRX_IRQ_AMI        _BV(5)
    00443
    00445 #define TRX_IRQ_UR         _BV(6)
    00446
    00448 #define TRX_IRQ_BAT_LOW    _BV(7)
    00449
    00451 #define TRAC_SUCCESS (0)
    00452
    00453 #define TRAC_CHANNEL_ACCESS_FAILURE (3)
    00454
    00455 #define TRAC_NO_ACK (5)
    00456
    00457
    00459 #define TRX_MIN_CHANNEL (0)
    00460
    00462 #define TRX_MAX_CHANNEL (10)
    00463
    00465 #define TRX_NB_CHANNELS (11)
    00466
    00472 #define TRX_SUPPORTED_CHANNELS  (0x00007ffUL)
    00473
    00478 #define TRX_SUPPORTED_PAGES     (42)
    00479 #define TRX_SUPPORTS_BAND_700 (1)
    00480 #define TRX_SUPPORTS_BAND_800 (1)
    00481 #define TRX_SUPPORTS_BAND_900 (1)
    00482
    00484 #define TRX_BPSK20    (0)
    00485
    00487 #define TRX_BPSK40    (4)
    00488
    00490 #define TRX_OQPSK100  (8)
    00491
    00493 #define TRX_OQPSK200  (9)
    00494
    00496 #define TRX_OQPSK400  (10)
    00497 #define TRX_OQPSK400_1  (11)
    00498
    00500 #define TRX_OQPSK250  (12)
    00501
    00503 #define TRX_OQPSK500  (13)
    00504
    00506 #define TRX_OQPSK1000 (14)
    00507 #define TRX_OQPSK1000_1 (15)
    00508
    00509 #define TRX_NONE      (255)
    00510
    00511 #endif /* ifndef AT86RF212_H */