Defines

# board_stbrfa1.h File Reference

This board is describes the Sensor Terminal Board from Dresden Electronic. It is a carrier board for the RCB family. More...

Go to the source code of this file.

## Defines
#define | DEFAULT_SPI_RATE (SPI_RATE_1_2)
#define | FT245_DDR DDRE
#define | FT245_INIT()
#define | FT245_PIN PINE
#define | FT245_RX_DATA() ((FT245_PIN & FT245_RXF))
#define | FT245_RXF _BV(7)
#define | FT245_TX_DATA() ((FT245_PIN & FT245_TXE))
#define | FT245_TXE _BV(6)
#define | HIF_IO_ENABLE hif_mmio_init
#define | HIF_NO_DATA (0x0100)
#define | HIF_TYPE (HIF_FT245)
#define | HIF_USB_READ() hif_usb_read()
#define | HIF_USB_WRITE(x) hif_usb_write(x)
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL+1)
#define | HWTMR_PRESCALE (1)
#define | INVERSE_KEYS (0)
#define | KEY_INIT hif_mmio_init
#define | LED_CLR(ln)
#define | LED_GET_VALUE() ((~LED_SHADOW & LED_MASK) >> LED_SHIFT)
#define | LED_INIT()
#define | LED_MASK (0x03)
#define | LED_NUMBER (2)
#define | LED_SET(ln)
#define | LED_SET_VALUE(x)
#define | LED_SHADOW GPIOR2
#define | LED_SHIFT (0)
#define | LED_TOGGLE(ln)
#define | LED_VAL(msk, val)
#define | LEDS_INVERSE (1)
#define | MASK_KEY (0x1)
#define | PIN_KEY (hif_key_read())
#define | PULLUP_KEYS (0)
#define | RX_HAS_DATA (0)
#define | RX_HAS_NO_DATA (FT245_RXF)
#define | SHIFT_KEY (0)
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_OVF_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TX_IS_BLOCKED (FT245_TXE)
#define | TX_IS_READY (0)

## Detailed Description

This board is describes the Sensor Terminal Board from Dresden Electronic. It is a carrier board for the RCB family.

The Sensor Terminal Board is a carrier board for the radio controller board family.

The wiring of this module is very specific; normally, all the functionality on the Sensor Terminal Board (FTDI, LEDs, button) is controlled by memory-mapped IO, using the external memory interface of the ATmegas. This is not possible with the ATmega128RFA1 as it does not feature an external memory interface. For that reason, GPIO lines have been re-wired to allow an external memory interface emulation. The schematics of the RCB128RFA1 document the following wiring:

    RCB2xx        | Pin           | RCB128RFA1   | Remark
    ------------------------------------------------------------------
    PA0             EXT1.23         PB0          \
    PA1             EXT1.24         PB1          |  This is the
    PA2             EXT1.25         PB2          |  multiplexed
    PA3             EXT1.26         PB3          >  data/low address
    PA4             EXT1.27         PB4          |  bus of the classic
    PA5             EXT1.28         PB5          |  XMEM interface
    PA6             EXT1.29         PB6          |
    PA7             EXT1.30         PB7          /
    PE4             EXT1.6          RSTON        Reset output
    PE5             EXT1.5          TST          Used for "HV" prog
    PC4             EXT0.25         PD4          \  Matches A12...A15
    PC5             EXT0.26         PD5          |  of normal address bus;
    PC6             EXT0.27         PD6          >  used to distinguish
    PC7             EXT0.28         PD7          /  FTDI vs. LED vs. button
    PG0             EXT0.17         PE4          xmem /WR
    PG1             EXT0.18         PE5          xmem /RD
    PB6             EXT0.1          PG0          GPIO
    PB7             EXT0.2          PG1          GPIO
    XTAL1           EXT0.7          CLKI

In addition, the standard STB pin mapping is retained for:

PE7 FT245 /RXF PE6 FT245 /TXE PG2 ALE

The STBxxx has memory mapped LEDS and Keys. KEY: memory mapped on external memory bus address 0x4000 LEDS

- 2 x memory mapped at 0x4000 (Option 1)
- 3 x IO mapped at PE2:PE4 (Option 2)

You can select between using the LEDs on the RCB or on the STB. In order to use the RCB LEDS, you have to define the macro USE_RCB_LEDS.

The LEDs on STB have a write-only memory interface, so we can't read back the LED status. So we need to have a shadow register, which stores the current LED state. Since the board interface consists only of a header file, we use register GPIO2 on ATmega128RFA1 for shadowing, because it would be hard to ensure the single instantiation of a global variable from a header file, which is used in many module files.

Fuses/Locks: LF: 0xe2 - 8MHz internal RC Osc. HF: 0x11 - without boot loader HF: 0x10 - with boot loader EF: 0xff LOCK: 0xef - protection of boot section

Original Settings w/ rdk231 LF: 0x61 HF: 0x91 EF: 0xfe

Bootloader: Start at byte=0x1e000, address=0xf000, size = 4096 instructions/ 8192 bytes

Build Options

- stb128rfa1 : STB + RCB128RFA1

## Define Documentation

#define DEFAULT_SPI_RATE (SPI_RATE_1_2)

ID String for this hardware

#define FT245_INIT | ( |  | ) |

Value:

    do { \
               FT245_DDR &= ~(FT245_TXE|FT245_RXF);\
            } while(0)

#define LED_CLR | ( |  | ln | ) |

Value:

    do{\
                LED_SHADOW |= (_BV(ln+LED_SHIFT) & LED_MASK);\
                hif_led_write(LED_SHADOW);\
            }while(0)

#define LED_INIT | ( |  | ) |

Value:

    do{\
                hif_mmio_init(); \
                LED_SHADOW = LED_MASK;\
                hif_led_write(LED_SHADOW);        \
            }while(0)

#define LED_SET | ( |  | ln | ) |

Value:

    do{\
                LED_SHADOW &= ~(_BV(ln+LED_SHIFT) & LED_MASK);\
                hif_led_write(LED_SHADOW);\
            }while(0)

#define LED_SET_VALUE | ( |  | x | ) |

Value:

    do{\
                LED_SHADOW = (LED_SHADOW & ~LED_MASK) | ((~x<<LED_SHIFT) & LED_MASK);\
                hif_led_write(LED_SHADOW);\
            }while(0)

#define LED_TOGGLE | ( |  | ln | ) |

Value:

    do{\
                LED_SHADOW ^= (_BV(ln+LED_SHIFT) & LED_MASK);\
                hif_led_write(LED_SHADOW);\
            }while(0)

#define LED_VAL | ( |  | msk,
|  |  | val |
| ) |  |  |

Value:

    do{\
                LED_SHADOW &= ~(LED_MASK|(msk<<LED_SHIFT)); \
                LED_SHADOW |= ~(val & (LED_MASK|msk));\
                hif_led_write(LED_SHADOW);\
            }while(0)

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= _BV(CS10); \
            TIMSK1 |= _BV(TOIE1); \
        }while(0)

Intialization of the hardware timer T1 (16bit)

- CS1[2:0] = 1 : Prescaler = 1
- WGM1[3:0] = 0 : Mode = 4 : CTC operation

Timer is clocked at F_CPU, and TIMER_IRQ_vect is called every 65535 ticks.

#define TIMER_IRQ_vect TIMER1_OVF_vect

Vector for Timer IRQ routine