Defines

# board_ict_11.h File Reference

Definition 2.4G Module from In-Circquit with AT86RF230B and Atmega1281 (V1.1). More...

Go to the source code of this file.

## Defines
#define | CUSTOM_RESET_TIME_MS (10)
#define | DEFAULT_SPI_RATE (SPI_RATE_1_4)
#define | HIF_TYPE HIF_UART_1
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL)
#define | HWTMR_PRESCALE (1)
#define | LED_DDR DDRG
#define | LED_MASK (0x20)
#define | LED_NUMBER (1)
#define | LED_PORT PORTG
#define | LED_SHIFT (5)
#define | LEDS_INVERSE (1)
#define | NO_KEYS (1)
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)

## Detailed Description

Definition 2.4G Module from In-Circquit with AT86RF230B and Atmega1281 (V1.1).

The wiring of the radio and the ATmega is shown below:

      ATmega1281    AT86RF230
      ----------    ---------
        PB1    --> SCK
        PB2    <-- MOSI
        PB3    --> MISO
        PB0    --> SEL
        PB4    --> SLP_TR
        PB5    --> TRX_RESET
        PD4/ICP1  --> IRQ
        PD6/T1   <-- CLKM

        PG5   --> LED Interface

        Fuses:
          LF: 0xe2 - 8MHz internal RC Osc.
          HF: 0x11 - without boot loader
          HF: 0x10 - with boot loader
          EF: 0xff
          LOCK: 0xef - protection of boot section

        Original Fuse settings (Stick):
           LF: 0xe2
           HF: 0x1a
           EF: 0xfd

        Original Fuse settings (Module):
           LF: 0x62
           HF: 0x93
           EF: 0xff

    Bootloader:
        Start at byte=0x1e000, address=0xf000, size = 4096 instructions/ 8192 bytes

Build Options
  - In-Cirquit radio stick
    - ics230_11 : version 1.1 (RF230 RevB)
    - ics230_12 : version 1.2 (RF230 RevB; AtMega128)
  - In-Cirquit radio module
    - icm230_11 : version 1.1 (RF230 RevB)
    - icm230_12a : version 1.2 (RF230 RevA) [shiny finish]
    - icm230_12b : version 1.2 (RF230 RevB) [tarnished finish]
    - icm230_12c : version 1.2 (RF230 RevB) [tarnished finish & AtMega128]

## Define Documentation

#define CUSTOM_RESET_TIME_MS (10)

additional delay needed by hardware

#define DEFAULT_SPI_RATE (SPI_RATE_1_4)

ID String for this hardware