# board_ict_11.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2009-2011, Bjoern Riemer, Karl Fessel, Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id$ */
    00030
    00088 #if defined(ics230_11)
    00089 # define BOARD_NAME "icstick230"
    00090 # define BOARD_TYPE (BOARD_ICS230_11)
    00091 # define RADIO_TYPE (RADIO_AT86RF230B)
    00092
    00093 #elif defined(icm230_11)
    00094 # define BOARD_NAME "icmodule230"
    00095 # define BOARD_TYPE (BOARD_ICM230_11)
    00096 # define RADIO_TYPE (RADIO_AT86RF230B)
    00097
    00098 #elif defined(icm230_12a)
    00099 # define BOARD_NAME "icmodule230a"
    00100 # define BOARD_TYPE (BOARD_ICM230_12A)
    00101 # define RADIO_TYPE (RADIO_AT86RF230A)
    00102
    00103 #elif defined(icm230_12b)
    00104 # define BOARD_NAME "icmodule230b"
    00105 # define BOARD_TYPE (BOARD_ICM230_12B)
    00106 # define RADIO_TYPE (RADIO_AT86RF230B)
    00107
    00108 #elif defined(icm230_12c)
    00109 # define BOARD_NAME "icmodule230c"
    00110 # define BOARD_TYPE (BOARD_ICM230_12C)
    00111 # define RADIO_TYPE (RADIO_AT86RF230B)
    00112
    00113 #elif defined(ics230_12)
    00114 # define BOARD_NAME "icstick230_12"
    00115 # define BOARD_TYPE (BOARD_ICS230_12)
    00116 # define RADIO_TYPE (RADIO_AT86RF230B)
    00117 #endif
    00118
    00119 #ifndef BOARD_ICT230_11_H
    00120 #define BOARD_ICT230_11_H
    00121
    00122 /*=== Compile time parameters ========================================*/
    00123 #ifndef DEFAULT_SPI_RATE
    00124 # define DEFAULT_SPI_RATE  (SPI_RATE_1_4)
    00125 #endif
    00126
    00127 /*=== Hardware Components ============================================*/
    00128
    00129 /*=== TRX pin access macros ==========================================*/
    00130 #if defined(__AVR_ATmega1281__)
    00131 # include "base_rdk230.h"
    00132 #elif defined(__AVR_ATmega128__)
    00133 # include "base_rdk230_m128.h"
    00134 #endif
    00135
    00136 #define CUSTOM_RESET_TIME_MS (10)
    00138 /*=== LED access macros ==============================================*/
    00139
    00140 /* stick settings */
    00141 #if (BOARD_TYPE == BOARD_ICS230_11) || (BOARD_TYPE == BOARD_ICS230_12)
    00142 # define LED_PORT      PORTG
    00143 # define LED_DDR       DDRG
    00144 # define LED_MASK      (0x20)
    00145 # define LED_SHIFT     (5)
    00146 # define LEDS_INVERSE  (1)
    00147 # define LED_NUMBER    (1)
    00148 #elif BOARD_TYPE == BOARD_ICM230_11
    00149 # define LED_PORT      PORTD
    00150 # define LED_DDR       DDRD
    00151 # define LED_MASK      (0xc0)
    00152 # define LED_SHIFT     (6)
    00153 # define LEDS_INVERSE  (1)
    00154 # define LED_NUMBER    (2)
    00155 #elif (BOARD_TYPE == BOARD_ICM230_12A) ||\
    00156       (BOARD_TYPE == BOARD_ICM230_12B) ||\
    00157       (BOARD_TYPE == BOARD_ICM230_12C)
    00158 # define LED_PORT      PORTA
    00159 # define LED_DDR       DDRA
    00160 # define LED_MASK      (_BV(4)|_BV(5)|_BV(6)|_BV(7))
    00161 # define LED_SHIFT     (4)
    00162 # define LEDS_INVERSE  (0)
    00163 # define LED_NUMBER    (4)
    00164 #endif
    00165
    00166
    00167 /*=== KEY access macros ==============================================*/
    00168 #if (BOARD_TYPE == BOARD_ICS230_11) || (BOARD_TYPE == BOARD_ICS230_12)
    00169 # define NO_KEYS (1)
    00170 #elif (BOARD_TYPE == BOARD_ICM230_11) ||\
    00171       (BOARD_TYPE == BOARD_ICM230_12A) ||\
    00172       (BOARD_TYPE == BOARD_ICM230_12B) ||\
    00173       (BOARD_TYPE == BOARD_ICM230_12C)
    00174 # define PORT_KEY     PORTD
    00175 # define PIN_KEY      PIND
    00176 # define DDR_KEY      DDRD
    00177 # define MASK_KEY     (0x01)
    00178 # define SHIFT_KEY    (0)
    00179 # define INVERSE_KEYS (1)
    00180 # define PULLUP_KEYS  (1)
    00181 #endif
    00182
    00183 /*=== Host Interface ================================================*/
    00184 # define HIF_TYPE    HIF_UART_1
    00185
    00186 /*=== TIMER Interface ===============================================*/
    00187 #define HWTMR_PRESCALE  (1)
    00188 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00189 #define HWTIMER_TICK_NB (0xFFFFUL)
    00190 #define HWTIMER_REG     (TCNT1)
    00191 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00192 #define TIMER_POOL_SIZE (4)
    00193
    00194 #if defined(__AVR_ATmega1281__)
    00195 # define TIMER_INIT() \
    00196     do{ \
    00197         TCCR1B |= (_BV(CS10)); \
    00198         TIMSK1 |= _BV(TOIE1); \
    00199     }while(0)
    00200
    00201 # define TIMER_IRQ_vect   TIMER1_OVF_vect
    00202 #elif defined(__AVR_ATmega128__)
    00203 # define TIMER_INIT() \
    00204     do{ \
    00205         TCCR1B |= (_BV(CS10)); \
    00206         TIMSK |= _BV(TOIE1); \
    00207     }while(0)
    00208
    00209 # define TIMER_IRQ_vect   TIMER1_OVF_vect
    00210 #endif
    00211
    00212 #endif /* BOARD_ICT230_11_H */