# Todo List

page µracoli Library User Guide
  Finish the construction work

Global LED_VAL
  how to implement this?

Global trx_frame_read_crc
  implement this function

Global trx_frame_read_data_crc
  implement this function

Global SUCCESS
  same like CCA_FREE, include/avr/iom128rfa1.h:3687:define SUCCESS

Global rxidle_t
  make it state_t variable, so that idle state can explicitely selected.

Page Libraries
  describe structure and concept of the libraries