# at86rf230b.h File Reference

## Detailed Description

AT86RF230 Rev.B 2.4GHz IEEE 802.15.4-Transceiver.

Definition in file at86rf230b.h.

Go to the source code of this file.

## Defines
#define | AT86RF230B_H (1)
#define | BUSY_RX (1)
#define | BUSY_RX_AACK (17)
#define | BUSY_RX_AACK_NOCLK (30)
#define | BUSY_TX (2)
#define | BUSY_TX_ARET (18)
#define | CLKM_16MHz (5)
#define | CLKM_1MHz (1)
#define | CLKM_2mA (0)
#define | CLKM_2MHz (2)
#define | CLKM_4mA (1)
#define | CLKM_4MHz (3)
#define | CLKM_6mA (2)
#define | CLKM_8mA (3)
#define | CLKM_8MHz (4)
#define | CLKM_no_clock (0)
#define | CMD_FORCE_TRX_OFF (3)
#define | CMD_NOP (0)
#define | CMD_PLL_ON (9)
#define | CMD_RX_AACK_ON (22)
#define | CMD_RX_ON (6)
#define | CMD_TRX_OFF (8)
#define | CMD_TX_ARET_ON (25)
#define | CMD_TX_START (2)
#define | P_ON (0)
#define | PLL_ON (9)
#define | RADIO_NAME "AT86RF230B"
#define | RADIO_PART_NUM (RF230B_PART_NUM)
#define | RADIO_VERSION_NUM (RF230B_VERSION_NUM)
#define | RATE_CODE_NONE (255)
#define | RATE_CODE_OQPSK250 (0)
#define | RF230B_PART_NUM (2)
#define | RF230B_VERSION_NUM (2)
#define | RG_BATMON (0x11)
#define | RG_CCA_THRES (0x9)
#define | RG_CSMA_SEED_0 (0x2d)
#define | RG_CSMA_SEED_1 (0x2e)
#define | RG_IEEE_ADDR_0 (0x24)
#define | RG_IEEE_ADDR_1 (0x25)
#define | RG_IEEE_ADDR_2 (0x26)
#define | RG_IEEE_ADDR_3 (0x27)
#define | RG_IEEE_ADDR_4 (0x28)
#define | RG_IEEE_ADDR_5 (0x29)
#define | RG_IEEE_ADDR_6 (0x2a)
#define | RG_IEEE_ADDR_7 (0x2b)
#define | RG_IRQ_MASK (0xe)
#define | RG_IRQ_STATUS (0xf)
#define | RG_MAN_ID_0 (0x1e)
#define | RG_MAN_ID_1 (0x1f)
#define | RG_PAN_ID_0 (0x22)
#define | RG_PAN_ID_1 (0x23)
#define | RG_PART_NUM (0x1c)
#define | RG_PHY_CC_CCA (0x8)
#define | RG_PHY_ED_LEVEL (0x7)
#define | RG_PHY_RSSI (0x6)
#define | RG_PHY_TX_PWR (0x5)
#define | RG_PLL_CF (0x1a)
#define | RG_PLL_DCU (0x1b)
#define | RG_SHORT_ADDR_0 (0x20)
#define | RG_SHORT_ADDR_1 (0x21)
#define | RG_TRX_CTRL_0 (0x3)
#define | RG_TRX_STATE (0x2)
#define | RG_TRX_STATUS (0x1)
#define | RG_VERSION_NUM (0x1d)
#define | RG_VREG_CTRL (0x10)
#define | RG_XAH_CTRL (0x2c)
#define | RG_XOSC_CTRL (0x12)
#define | RX_AACK_ON (22)
#define | RX_AACK_ON_NOCLK (29)
#define | RX_ON (6)
#define | RX_ON_NOCLK (28)
#define | SLEEP (15)
#define | SR_AACK_I_AM_COORD 0x2e,0x8,3
#define | SR_AACK_SET_PD 0x2e,0x20,5
#define | SR_AVDD_OK 0x10,0x40,6
#define | SR_AVREG_EXT 0x10,0x80,7
#define | SR_BAT_LOW 0xf,0x80,7
#define | SR_BATMON_HR 0x11,0x10,4
#define | SR_BATMON_OK 0x11,0x20,5
#define | SR_BATMON_VTH 0x11,0xf,0
#define | SR_CCA_DONE 0x1,0x80,7
#define | SR_CCA_ED_THRES 0x9,0xf,0
#define | SR_CCA_MODE 0x8,0x60,5
#define | SR_CCA_REQUEST 0x8,0x80,7
#define | SR_CCA_STATUS 0x1,0x40,6
#define | SR_CHANNEL 0x8,0x1f,0
#define | SR_CLKM_CTRL 0x3,0x7,0
#define | SR_CLKM_SHA_SEL 0x3,0x8,3
#define | SR_CSMA_SEED_0 0x2d,0xff,0
#define | SR_CSMA_SEED_1 0x2e,0x7,0
#define | SR_DVDD_OK 0x10,0x4,2
#define | SR_DVREG_EXT 0x10,0x8,3
#define | SR_ED_LEVEL 0x7,0xff,0
#define | SR_IEEE_ADDR_0 0x24,0xff,0
#define | SR_IEEE_ADDR_1 0x25,0xff,0
#define | SR_IEEE_ADDR_2 0x26,0xff,0
#define | SR_IEEE_ADDR_3 0x27,0xff,0
#define | SR_IEEE_ADDR_4 0x28,0xff,0
#define | SR_IEEE_ADDR_5 0x29,0xff,0
#define | SR_IEEE_ADDR_6 0x2a,0xff,0
#define | SR_IEEE_ADDR_7 0x2b,0xff,0
#define | SR_MAN_ID_0 0x1e,0xff,0
#define | SR_MAN_ID_1 0x1f,0xff,0
#define | SR_MASK_BAT_LOW 0xe,0x80,7
#define | SR_MASK_PLL_UNLOCK 0xe,0x3,0
#define | SR_MASK_TRX_END 0xe,0x8,3
#define | SR_MASK_TRX_START 0xe,0x4,2
#define | SR_MASK_TRX_UR 0xe,0x40,6
#define | SR_MAX_CSMA_RETRIES 0x2c,0xf,0
#define | SR_MAX_FRAME_RETRIES 0x2c,0xf0,4
#define | SR_MIN_BE 0x2e,0xc0,6
#define | SR_PAD_IO 0x3,0xc0,6
#define | SR_PAD_IO_CLKM 0x3,0x30,4
#define | SR_PAN_ID_0 0x22,0xff,0
#define | SR_PAN_ID_1 0x23,0xff,0
#define | SR_PART_NUM 0x1c,0xff,0
#define | SR_PLL_CF_START 0x1a,0x80,7
#define | SR_PLL_DCU_START 0x1b,0x80,7
#define | SR_PLL_UNLOCK 0xf,0x3,0
#define | SR_RSSI 0x6,0x1f,0
#define | SR_RX_CRC_VALID 0x6,0x80,7
#define | SR_RX_END 0xf,0x8,3
#define | SR_RX_START 0xf,0x4,2
#define | SR_SHORT_ADDR_0 0x20,0xff,0
#define | SR_SHORT_ADDR_1 0x21,0xff,0
#define | SR_TRAC_STATUS 0x2,0xe0,5
#define | SR_TRX_CMD 0x2,0x1f,0
#define | SR_TRX_STATUS 0x1,0x1f,0
#define | SR_TRX_UR 0xf,0x40,6
#define | SR_TX_AUTO_CRC_ON 0x5,0x80,7
#define | SR_TX_PWR 0x5,0xf,0
#define | SR_VERSION_NUM 0x1d,0xff,0
#define | SR_XTAL_MODE 0x12,0xf0,4
#define | SR_XTAL_TRIM 0x12,0xf,0
#define | TRAC_CHANNEL_ACCESS_FAILURE (3)
#define | TRAC_INVALID (7)
#define | TRAC_NO_ACK (5)
#define | TRAC_SUCCESS (0)
#define | TRAC_SUCCESS_DATA_PENDING (1)
#define | TRX_CCA_TIME_US (140)
#define | TRX_CMD_FR (_BV(5))
#define | TRX_CMD_FW (_BV(6) | _BV(5))
#define | TRX_CMD_RADDR_MASK (0x3f)
#define | TRX_CMD_RR (_BV(7))
#define | TRX_CMD_RW (_BV(7) | _BV(6))
#define | TRX_CMD_SR (0)
#define | TRX_CMD_SW (_BV(6))
#define | TRX_INIT_TIME_US (510)
#define | TRX_IRQ_BAT_LOW _BV(7)
#define | TRX_IRQ_PLL_LOCK _BV(0)
#define | TRX_IRQ_PLL_UNLOCK _BV(1)
#define | TRX_IRQ_RX_START _BV(2)
#define | TRX_IRQ_TRX_END _BV(3)
#define | TRX_IRQ_UR _BV(6)
#define | TRX_MAX_CHANNEL (26)
#define | TRX_MIN_CHANNEL (11)
#define | TRX_NB_CHANNELS (16)
#define | TRX_OFF (8)
#define | TRX_PLL_LOCK_TIME_US (180)
#define | TRX_RESET_TIME_US (6)
#define | TRX_SUPPORTED_CHANNELS (0x7fff800UL)
| Mask for supported channels of this radio. The AT86RF230 supports channels 11 ... 26 of IEEE 802.15.4.
#define | TRX_SUPPORTED_PAGES (42)
| Mask for supported channel pages (a.k.a. modulation schemes) of this radio. The AT86RF230 supports channel page ???? OQPSK_250.
#define | TRX_SUPPORTS_BAND_2400 (1)
#define | TX_ARET_ON (25)
## Typedefs
typedef uint8_t | trx_ramaddr_t
typedef uint8_t | trx_regaddr_t
typedef uint8_t | trx_regval_t

## Define Documentation

#define RADIO_NAME "AT86RF230B"

name string of the radio

Definition at line 283 of file at86rf230b.h.

#define RADIO_PART_NUM (RF230B_PART_NUM)

contents of the RG_PART_NUM register

Definition at line 285 of file at86rf230b.h.

#define RADIO_VERSION_NUM (RF230B_VERSION_NUM)

contents of the RG_VERSION_NUM register

Definition at line 287 of file at86rf230b.h.

#define RATE_CODE_NONE (255)

undefined data rate

Definition at line 364 of file at86rf230b.h.

#define RATE_CODE_OQPSK250 (0)

Rate code for OQPSK250, xx kchip/s, yy kbit/s

Definition at line 361 of file at86rf230b.h.

#define RG_BATMON (0x11)

Offset for register BATMON

Definition at line 175 of file at86rf230b.h.

#define RG_CCA_THRES (0x9)

Offset for register CCA_THRES

Definition at line 137 of file at86rf230b.h.

#define RG_CSMA_SEED_0 (0x2d)

Offset for register CSMA_SEED_0

Definition at line 269 of file at86rf230b.h.

#define RG_CSMA_SEED_1 (0x2e)

Offset for register CSMA_SEED_1

Definition at line 273 of file at86rf230b.h.

#define RG_IEEE_ADDR_0 (0x24)

Offset for register IEEE_ADDR_0

Definition at line 231 of file at86rf230b.h.

#define RG_IEEE_ADDR_1 (0x25)

Offset for register IEEE_ADDR_1

Definition at line 235 of file at86rf230b.h.

#define RG_IEEE_ADDR_2 (0x26)

Offset for register IEEE_ADDR_2

Definition at line 239 of file at86rf230b.h.

#define RG_IEEE_ADDR_3 (0x27)

Offset for register IEEE_ADDR_3

Definition at line 243 of file at86rf230b.h.

#define RG_IEEE_ADDR_4 (0x28)

Offset for register IEEE_ADDR_4

Definition at line 247 of file at86rf230b.h.

#define RG_IEEE_ADDR_5 (0x29)

Offset for register IEEE_ADDR_5

Definition at line 251 of file at86rf230b.h.

#define RG_IEEE_ADDR_6 (0x2a)

Offset for register IEEE_ADDR_6

Definition at line 255 of file at86rf230b.h.

#define RG_IEEE_ADDR_7 (0x2b)

Offset for register IEEE_ADDR_7

Definition at line 259 of file at86rf230b.h.

#define RG_IRQ_MASK (0xe)

Offset for register IRQ_MASK

Definition at line 141 of file at86rf230b.h.

#define RG_IRQ_STATUS (0xf)

Offset for register IRQ_STATUS

Definition at line 153 of file at86rf230b.h.

#define RG_MAN_ID_0 (0x1e)

Offset for register MAN_ID_0

Definition at line 207 of file at86rf230b.h.

#define RG_MAN_ID_1 (0x1f)

Offset for register MAN_ID_1

Definition at line 211 of file at86rf230b.h.

#define RG_PAN_ID_0 (0x22)

Offset for register PAN_ID_0

Definition at line 223 of file at86rf230b.h.

#define RG_PAN_ID_1 (0x23)

Offset for register PAN_ID_1

Definition at line 227 of file at86rf230b.h.

#define RG_PART_NUM (0x1c)

Offset for register PART_NUM

Definition at line 197 of file at86rf230b.h.

#define RG_PHY_CC_CCA (0x8)

Offset for register PHY_CC_CCA

Definition at line 129 of file at86rf230b.h.

#define RG_PHY_ED_LEVEL (0x7)

Offset for register PHY_ED_LEVEL

Definition at line 125 of file at86rf230b.h.

#define RG_PHY_RSSI (0x6)

Offset for register PHY_RSSI

Definition at line 119 of file at86rf230b.h.

#define RG_PHY_TX_PWR (0x5)

Offset for register PHY_TX_PWR

Definition at line 113 of file at86rf230b.h.

#define RG_PLL_CF (0x1a)

Offset for register PLL_CF

Definition at line 189 of file at86rf230b.h.

#define RG_PLL_DCU (0x1b)

Offset for register PLL_DCU

Definition at line 193 of file at86rf230b.h.

#define RG_SHORT_ADDR_0 (0x20)

Offset for register SHORT_ADDR_0

Definition at line 215 of file at86rf230b.h.

#define RG_SHORT_ADDR_1 (0x21)

Offset for register SHORT_ADDR_1

Definition at line 219 of file at86rf230b.h.

#define RG_TRX_CTRL_0 (0x3)

Offset for register TRX_CTRL_0

Definition at line 93 of file at86rf230b.h.

#define RG_TRX_STATE (0x2)

Offset for register TRX_STATE

Definition at line 74 of file at86rf230b.h.

#define RG_TRX_STATUS (0x1)

Offset for register TRX_STATUS

Definition at line 52 of file at86rf230b.h.

#define RG_VERSION_NUM (0x1d)

Offset for register VERSION_NUM

Definition at line 202 of file at86rf230b.h.

#define RG_VREG_CTRL (0x10)

Offset for register VREG_CTRL

Definition at line 165 of file at86rf230b.h.

#define RG_XAH_CTRL (0x2c)

Offset for register XAH_CTRL

Definition at line 263 of file at86rf230b.h.

#define RG_XOSC_CTRL (0x12)

Offset for register XOSC_CTRL

Definition at line 183 of file at86rf230b.h.

#define SR_AACK_I_AM_COORD 0x2e,0x8,3

Access parameters for sub-register AACK_I_AM_COORD in register CSMA_SEED_1

Definition at line 279 of file at86rf230b.h.

#define SR_AACK_SET_PD 0x2e,0x20,5

Access parameters for sub-register AACK_SET_PD in register CSMA_SEED_1

Definition at line 277 of file at86rf230b.h.

#define SR_AVDD_OK 0x10,0x40,6

Access parameters for sub-register AVDD_OK in register VREG_CTRL

Definition at line 169 of file at86rf230b.h.

#define SR_AVREG_EXT 0x10,0x80,7

Access parameters for sub-register AVREG_EXT in register VREG_CTRL

Definition at line 167 of file at86rf230b.h.

#define SR_BAT_LOW 0xf,0x80,7

Access parameters for sub-register BAT_LOW in register IRQ_STATUS

Definition at line 155 of file at86rf230b.h.

#define SR_BATMON_HR 0x11,0x10,4

Access parameters for sub-register BATMON_HR in register BATMON

Definition at line 179 of file at86rf230b.h.

#define SR_BATMON_OK 0x11,0x20,5

Access parameters for sub-register BATMON_OK in register BATMON

Definition at line 177 of file at86rf230b.h.

#define SR_BATMON_VTH 0x11,0xf,0

Access parameters for sub-register BATMON_VTH in register BATMON

Definition at line 181 of file at86rf230b.h.

#define SR_CCA_DONE 0x1,0x80,7

Access parameters for sub-register CCA_DONE in register TRX_STATUS

Definition at line 54 of file at86rf230b.h.

#define SR_CCA_ED_THRES 0x9,0xf,0

Access parameters for sub-register CCA_ED_THRES in register CCA_THRES

Definition at line 139 of file at86rf230b.h.

#define SR_CCA_MODE 0x8,0x60,5

Access parameters for sub-register CCA_MODE in register PHY_CC_CCA

Definition at line 133 of file at86rf230b.h.

#define SR_CCA_REQUEST 0x8,0x80,7

Access parameters for sub-register CCA_REQUEST in register PHY_CC_CCA

Definition at line 131 of file at86rf230b.h.

#define SR_CCA_STATUS 0x1,0x40,6

Access parameters for sub-register CCA_STATUS in register TRX_STATUS

Definition at line 56 of file at86rf230b.h.

#define SR_CHANNEL 0x8,0x1f,0

Access parameters for sub-register CHANNEL in register PHY_CC_CCA

Definition at line 135 of file at86rf230b.h.

#define SR_CLKM_CTRL 0x3,0x7,0

Access parameters for sub-register CLKM_CTRL in register TRX_CTRL_0

Definition at line 105 of file at86rf230b.h.

#define SR_CLKM_SHA_SEL 0x3,0x8,3

Access parameters for sub-register CLKM_SHA_SEL in register TRX_CTRL_0

Definition at line 103 of file at86rf230b.h.

#define SR_CSMA_SEED_0 0x2d,0xff,0

Access parameters for sub-register CSMA_SEED_0 in register CSMA_SEED_0

Definition at line 271 of file at86rf230b.h.

#define SR_CSMA_SEED_1 0x2e,0x7,0

Access parameters for sub-register CSMA_SEED_1 in register CSMA_SEED_1

Definition at line 281 of file at86rf230b.h.

#define SR_DVDD_OK 0x10,0x4,2

Access parameters for sub-register DVDD_OK in register VREG_CTRL

Definition at line 173 of file at86rf230b.h.

#define SR_DVREG_EXT 0x10,0x8,3

Access parameters for sub-register DVREG_EXT in register VREG_CTRL

Definition at line 171 of file at86rf230b.h.

#define SR_ED_LEVEL 0x7,0xff,0

Access parameters for sub-register ED_LEVEL in register PHY_ED_LEVEL

Definition at line 127 of file at86rf230b.h.

#define SR_IEEE_ADDR_0 0x24,0xff,0

Access parameters for sub-register IEEE_ADDR_0 in register IEEE_ADDR_0

Definition at line 233 of file at86rf230b.h.

#define SR_IEEE_ADDR_1 0x25,0xff,0

Access parameters for sub-register IEEE_ADDR_1 in register IEEE_ADDR_1

Definition at line 237 of file at86rf230b.h.

#define SR_IEEE_ADDR_2 0x26,0xff,0

Access parameters for sub-register IEEE_ADDR_2 in register IEEE_ADDR_2

Definition at line 241 of file at86rf230b.h.

#define SR_IEEE_ADDR_3 0x27,0xff,0

Access parameters for sub-register IEEE_ADDR_3 in register IEEE_ADDR_3

Definition at line 245 of file at86rf230b.h.

#define SR_IEEE_ADDR_4 0x28,0xff,0

Access parameters for sub-register IEEE_ADDR_4 in register IEEE_ADDR_4

Definition at line 249 of file at86rf230b.h.

#define SR_IEEE_ADDR_5 0x29,0xff,0

Access parameters for sub-register IEEE_ADDR_5 in register IEEE_ADDR_5

Definition at line 253 of file at86rf230b.h.

#define SR_IEEE_ADDR_6 0x2a,0xff,0

Access parameters for sub-register IEEE_ADDR_6 in register IEEE_ADDR_6

Definition at line 257 of file at86rf230b.h.

#define SR_IEEE_ADDR_7 0x2b,0xff,0

Access parameters for sub-register IEEE_ADDR_7 in register IEEE_ADDR_7

Definition at line 261 of file at86rf230b.h.

#define SR_MAN_ID_0 0x1e,0xff,0

Access parameters for sub-register MAN_ID_0 in register MAN_ID_0

Definition at line 209 of file at86rf230b.h.

#define SR_MAN_ID_1 0x1f,0xff,0

Access parameters for sub-register MAN_ID_1 in register MAN_ID_1

Definition at line 213 of file at86rf230b.h.

#define SR_MASK_BAT_LOW 0xe,0x80,7

Access parameters for sub-register MASK_BAT_LOW in register IRQ_MASK

Definition at line 143 of file at86rf230b.h.

#define SR_MASK_PLL_UNLOCK 0xe,0x3,0

Access parameters for sub-register MASK_PLL_UNLOCK in register IRQ_MASK

Definition at line 151 of file at86rf230b.h.

#define SR_MASK_TRX_END 0xe,0x8,3

Access parameters for sub-register MASK_TRX_END in register IRQ_MASK

Definition at line 147 of file at86rf230b.h.

#define SR_MASK_TRX_START 0xe,0x4,2

Access parameters for sub-register MASK_TRX_START in register IRQ_MASK

Definition at line 149 of file at86rf230b.h.

#define SR_MASK_TRX_UR 0xe,0x40,6

Access parameters for sub-register MASK_TRX_UR in register IRQ_MASK

Definition at line 145 of file at86rf230b.h.

#define SR_MAX_CSMA_RETRIES 0x2c,0xf,0

Access parameters for sub-register MAX_CSMA_RETRIES in register XAH_CTRL

Definition at line 267 of file at86rf230b.h.

#define SR_MAX_FRAME_RETRIES 0x2c,0xf0,4

Access parameters for sub-register MAX_FRAME_RETRIES in register XAH_CTRL

Definition at line 265 of file at86rf230b.h.

#define SR_MIN_BE 0x2e,0xc0,6

Access parameters for sub-register MIN_BE in register CSMA_SEED_1

Definition at line 275 of file at86rf230b.h.

#define SR_PAD_IO 0x3,0xc0,6

Access parameters for sub-register PAD_IO in register TRX_CTRL_0

Definition at line 95 of file at86rf230b.h.

#define SR_PAD_IO_CLKM 0x3,0x30,4

Access parameters for sub-register PAD_IO_CLKM in register TRX_CTRL_0

Definition at line 97 of file at86rf230b.h.

#define SR_PAN_ID_0 0x22,0xff,0

Access parameters for sub-register PAN_ID_0 in register PAN_ID_0

Definition at line 225 of file at86rf230b.h.

#define SR_PAN_ID_1 0x23,0xff,0

Access parameters for sub-register PAN_ID_1 in register PAN_ID_1

Definition at line 229 of file at86rf230b.h.

#define SR_PART_NUM 0x1c,0xff,0

Access parameters for sub-register PART_NUM in register PART_NUM

Definition at line 199 of file at86rf230b.h.

#define SR_PLL_CF_START 0x1a,0x80,7

Access parameters for sub-register PLL_CF_START in register PLL_CF

Definition at line 191 of file at86rf230b.h.

#define SR_PLL_DCU_START 0x1b,0x80,7

Access parameters for sub-register PLL_DCU_START in register PLL_DCU

Definition at line 195 of file at86rf230b.h.

#define SR_PLL_UNLOCK 0xf,0x3,0

Access parameters for sub-register PLL_UNLOCK in register IRQ_STATUS

Definition at line 163 of file at86rf230b.h.

#define SR_RSSI 0x6,0x1f,0

Access parameters for sub-register RSSI in register PHY_RSSI

Definition at line 123 of file at86rf230b.h.

#define SR_RX_CRC_VALID 0x6,0x80,7

Access parameters for sub-register RX_CRC_VALID in register PHY_RSSI

Definition at line 121 of file at86rf230b.h.

#define SR_RX_END 0xf,0x8,3

Access parameters for sub-register RX_END in register IRQ_STATUS

Definition at line 159 of file at86rf230b.h.

#define SR_RX_START 0xf,0x4,2

Access parameters for sub-register RX_START in register IRQ_STATUS

Definition at line 161 of file at86rf230b.h.

#define SR_SHORT_ADDR_0 0x20,0xff,0

Access parameters for sub-register SHORT_ADDR_0 in register SHORT_ADDR_0

Definition at line 217 of file at86rf230b.h.

#define SR_SHORT_ADDR_1 0x21,0xff,0

Access parameters for sub-register SHORT_ADDR_1 in register SHORT_ADDR_1

Definition at line 221 of file at86rf230b.h.

#define SR_TRAC_STATUS 0x2,0xe0,5

Access parameters for sub-register TRAC_STATUS in register TRX_STATE

Definition at line 76 of file at86rf230b.h.

#define SR_TRX_CMD 0x2,0x1f,0

Access parameters for sub-register TRX_CMD in register TRX_STATE

Definition at line 83 of file at86rf230b.h.

#define SR_TRX_STATUS 0x1,0x1f,0

Access parameters for sub-register TRX_STATUS in register TRX_STATUS

Definition at line 58 of file at86rf230b.h.

#define SR_TRX_UR 0xf,0x40,6

Access parameters for sub-register TRX_UR in register IRQ_STATUS

Definition at line 157 of file at86rf230b.h.

#define SR_TX_AUTO_CRC_ON 0x5,0x80,7

Access parameters for sub-register TX_AUTO_CRC_ON in register PHY_TX_PWR

Definition at line 115 of file at86rf230b.h.

#define SR_TX_PWR 0x5,0xf,0

Access parameters for sub-register TX_PWR in register PHY_TX_PWR

Definition at line 117 of file at86rf230b.h.

#define SR_VERSION_NUM 0x1d,0xff,0

Access parameters for sub-register VERSION_NUM in register VERSION_NUM

Definition at line 204 of file at86rf230b.h.

#define SR_XTAL_MODE 0x12,0xf0,4

Access parameters for sub-register XTAL_MODE in register XOSC_CTRL

Definition at line 185 of file at86rf230b.h.

#define SR_XTAL_TRIM 0x12,0xf,0

Access parameters for sub-register XTAL_TRIM in register XOSC_CTRL

Definition at line 187 of file at86rf230b.h.

#define TRX_CCA_TIME_US (140)

duration of a CCA measurement

Definition at line 314 of file at86rf230b.h.

#define TRX_CMD_FR (_BV(5))

SPI command code for frame read

Definition at line 296 of file at86rf230b.h.

#define TRX_CMD_FW (_BV(6) | _BV(5))

SPI command code for frame write

Definition at line 294 of file at86rf230b.h.

#define TRX_CMD_RR (_BV(7))

SPI command code for register read

Definition at line 292 of file at86rf230b.h.

#define TRX_CMD_RW (_BV(7) | _BV(6))

SPI command code for register write

Definition at line 290 of file at86rf230b.h.

#define TRX_CMD_SR (0)

SPI command code for sram read

Definition at line 300 of file at86rf230b.h.

#define TRX_CMD_SW (_BV(6))

SPI command code for sram write

Definition at line 298 of file at86rf230b.h.

#define TRX_INIT_TIME_US (510)

duration transceiver reaches TRX_OFF for the first time

Definition at line 308 of file at86rf230b.h.

#define TRX_IRQ_BAT_LOW _BV(7)

Mask for battery low interrupt

Definition at line 332 of file at86rf230b.h.

#define TRX_IRQ_PLL_LOCK _BV(0)

Mask for PLL lock interrupt

Definition at line 317 of file at86rf230b.h.

#define TRX_IRQ_PLL_UNLOCK _BV(1)

Mask for PLL unlock interrupt

Definition at line 320 of file at86rf230b.h.

#define TRX_IRQ_RX_START _BV(2)

Mask for RX Start interrupt

Definition at line 323 of file at86rf230b.h.

#define TRX_IRQ_TRX_END _BV(3)

Mask for RX/TX end interrupt

Definition at line 326 of file at86rf230b.h.

#define TRX_IRQ_UR _BV(6)

Mask for RX/TX underrun interrupt

Definition at line 329 of file at86rf230b.h.

#define TRX_MAX_CHANNEL (26)

highest supported channel number

Definition at line 340 of file at86rf230b.h.

#define TRX_MIN_CHANNEL (11)

lowest supported channel number

Definition at line 337 of file at86rf230b.h.

#define TRX_NB_CHANNELS (16)

number of channels

Definition at line 343 of file at86rf230b.h.

#define TRX_PLL_LOCK_TIME_US (180)

maximum duration, which PLL needs to lock

Definition at line 311 of file at86rf230b.h.

#define TRX_RESET_TIME_US (6)

duration while reset=low is asserted

Definition at line 305 of file at86rf230b.h.

#define TRX_SUPPORTED_CHANNELS (0x7fff800UL)

Mask for supported channels of this radio. The AT86RF230 supports channels 11 ... 26 of IEEE 802.15.4.

Definition at line 349 of file at86rf230b.h.

#define TRX_SUPPORTED_PAGES (42)

Mask for supported channel pages (a.k.a. modulation schemes) of this radio. The AT86RF230 supports channel page ???? OQPSK_250.

Definition at line 357 of file at86rf230b.h.