- Main Page
- Related Pages
- Modules
- Data Structures
- Files

# board_stk541.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2007 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_stk541.h,v 1.16 2009/06/22 05:29:39 awachtler Exp $ */
    00088 #if defined(psk230)
    00089 # define BOARD_TYPE (PSK_230)
    00090 # define BOARD_NAME_STK541 "psk230"
    00091 # define RADIO_TYPE (RADIO_AT86RF230A)
    00092 #elif defined(psk230b)
    00093 # define BOARD_TYPE (PSK_230B)
    00094 # define BOARD_NAME_STK541 "psk230b"
    00095 # define RADIO_TYPE (RADIO_AT86RF230B)
    00096 #elif defined(psk231)
    00097 # define BOARD_TYPE (PSK_231)
    00098 # define BOARD_NAME_STK541 "psk231"
    00099 # define RADIO_TYPE (RADIO_AT86RF231)
    00100 #elif defined(psk212)
    00101 # define BOARD_TYPE (PSK_212)
    00102 # define BOARD_NAME_STK541 "psk212"
    00103 # define RADIO_TYPE (RADIO_AT86RF212)
    00104 #endif
    00105
    00106 #ifndef BOARD_STK541_H
    00107 #define BOARD_STK541_H
    00108
    00109 #define BOARD_NAME BOARD_NAME_STK541
    00110
    00111 /*=== Compile time parameters ========================================*/
    00112 #ifndef MAX_FRAME_SIZE
    00113 # define MAX_FRAME_SIZE (127)
    00114 #endif
    00115
    00116 #ifndef DEFAULT_SPI_RATE
    00117 # define DEFAULT_SPI_RATE  (SPI_RATE_1_2)
    00118 #endif
    00119
    00120 /*=== radio interface definition =====================================*/
    00121 #if BOARD_TYPE == PSK_230 || BOARD_TYPE == PSK_230B
    00122 # include "base_rdk230.h"
    00123 #else
    00124 # include "base_rdk2xx.h"
    00125 #endif
    00126
    00127 /*=== LED access macros ==============================================*/
    00128 #define LED_PORT      PORTE
    00129 #define LED_DDR       DDRE
    00130 #define LED_MASK      (0x1c)
    00131 #define LED_SHIFT     (2)
    00132 #define LEDS_INVERSE  (1)
    00133 #define LED_NUMBER    (3)
    00134 /*=== KEY access macros ==============================================*/
    00135 #define PORT_KEY      PORTE
    00136 #define PIN_KEY       PINE
    00137 #define DDR_KEY       DDRE
    00138 #define MASK_KEY      (0x20)
    00139 #define SHIFT_KEY     (5)
    00140 #define INVERSE_KEYS  (1)
    00141 #define PULLUP_KEYS   (1)
    00142
    00143 /*=== Host Interface ================================================*/
    00144 #define HIF_TYPE      (HIF_FT245)
    00145 #define HIF_IO_ENABLE XRAM_ENABLE
    00146
    00147 #define USB_FIFO_AD  0xF000
    00148 #define XRAM_ENABLE() XMCRA |= (1 << SRE); XMCRB = (1 << XMBK)
    00149 #define HIF_NO_DATA   (0x0100)
    00150 #define FT245_DDR    DDRE
    00151 #define FT245_PIN    PINE
    00152 #define FT245_TXE    _BV(6)
    00153 #define FT245_RXF    _BV(7)
    00154 #define FT245_INIT() do { \
    00155            FT245_DDR &= ~(FT245_TXE|FT245_RXF);\
    00156         } while(0)
    00157 #define TX_IS_READY        (0)
    00158 #define TX_IS_BLOCKED      (FT245_TXE)
    00159 #define RX_HAS_DATA        (0)
    00160 #define RX_HAS_NO_DATA     (FT245_RXF)
    00161 #define FT245_RX_DATA()  ((FT245_PIN & FT245_RXF))
    00162 #define FT245_TX_DATA()  ((FT245_PIN & FT245_TXE))
    00163
    00164 /*=== TIMER Interface ===============================================*/
    00165 #define HWTMR_PRESCALE  (1)
    00166 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00167 #define HWTIMER_TICK_NB (0xFFFFUL+1)
    00168 #define HWTIMER_REG     (TCNT1)
    00169 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00170 #define TIMER_POOL_SIZE (4)
    00171
    00173 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00174
    00184 # define TIMER_INIT() \
    00185     do{ \
    00186         TCCR1B |= (_BV(CS10));\
    00187         TIMSK1 |= _BV(TOIE1); \
    00188     }while(0)
    00189
    00190
    00191 # define DBG_PORT PORTD
    00192 # define DBG_DDR DDRD
    00193 # define DBG_PIN (1<<PD0)
    00194
    00195 /*=== OSCCAL tuning =================================================*/
    00196 #ifndef TUNED_OSCCAL
    00197 # define TUNED_OSCCAL (0xbf)  /* default is 0xb1, but @2.9V 0xbf is better */
    00198 #endif
    00199 #endif /* BOARD_STK541_H */