# radio_status_t Struct Reference
[Radio Access Functions]

## Detailed Description

Structure for storage of radio parameters.

Definition at line 194 of file radio.h.

## Data Fields
uint8_t | cca_mode
uint8_t | channel
radio_state_t | idle_state
uint8_t * | rxframe
uint8_t | rxframesz
uint8_t | rxlqi
uint8_t | rxrssi
radio_state_t | state
uint8_t | tx_pwr

## Field Documentation

uint8_t radio_status_t::cca_mode

Current cca mode.

Definition at line 199 of file radio.h.

uint8_t radio_status_t::channel

Current radio channel. (MIN_CHANNEL ... MAX_CHANNEL)

Definition at line 196 of file radio.h.

radio_state_t radio_status_t::idle_state

after TX go to idle state

Definition at line 201 of file radio.h.

uint8_t* radio_status_t::rxframe

Pointer for frame data storage.

Definition at line 204 of file radio.h.

uint8_t radio_status_t::rxframesz

Length of the buffer rxframesz

Definition at line 205 of file radio.h.

uint8_t radio_status_t::rxlqi

LQI value of last received frame.

Definition at line 203 of file radio.h.

uint8_t radio_status_t::rxrssi

RSSI value of last received frame (see also VOID_RSSI).

Definition at line 202 of file radio.h.

radio_state_t radio_status_t::state

Current transceiver state.

Definition at line 200 of file radio.h.

uint8_t radio_status_t::tx_pwr

Current transmit power.

Definition at line 198 of file radio.h.