- Main Page
- Related Pages
- Modules
- Data Structures
- Files

# board_wdba1281.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2008 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_wdba1281.h,v 1.8 2009/05/18 05:26:26 awachtler Exp $ */
    00094 #if defined(mnb900)
    00095 # define BOARD_NAME_MESHBEAN "mnb900"
    00096 # define RADIO_TYPE (RADIO_AT86RF212)
    00097 # define BOARD_TYPE_MESHBEAN (MNB_900)
    00098 #elif defined(wdba1281)
    00099 # define BOARD_NAME_MESHBEAN "wdba1281"
    00100 # define RADIO_TYPE (RADIO_AT86RF230B)
    00101 # define BOARD_TYPE_MESHBEAN (WDB_A1281)
    00102 #endif
    00103
    00104 #ifndef BOARD_WDBA1281_H
    00105 #define BOARD_WDBA1281_H
    00106
    00107 #define BOARD_TYPE  (BOARD_TYPE_MESHBEAN)
    00108 #define BOARD_NAME  BOARD_NAME_MESHBEAN
    00109
    00110 /*=== Compile time parameters ========================================*/
    00111 #ifndef MAX_FRAME_SIZE
    00112 # define MAX_FRAME_SIZE (127)
    00113 #endif
    00114
    00115 /*=== radio interface definition =====================================*/
    00116 #include "boards/base_zdma1281.h"
    00117
    00118 /*=== LED access macros ==============================================*/
    00119 #define LED_PORT PORTB
    00120 #define LED_DDR  DDRB
    00121 #define LED_MASK 0xe0
    00122 #define LED_SHIFT     (5)
    00123 #define LEDS_INVERSE  (0)
    00124 #define LED_NUMBER    (3)
    00126 /*=== KEY access macros ==============================================*/
    00127 #define PORT_KEY PORTE
    00128 #define PIN_KEY  PINE
    00129 #define DDR_KEY  DDRE
    00130
    00131 #define MASK_KEY     (0xc0)
    00132 #define SHIFT_KEY    (6)
    00133 #define INVERSE_KEYS (1)
    00134 #define PULLUP_KEYS  (1)
    00135
    00136 #define SLEEP_ON_KEY_INIT() do{}while(0)
    00137 #define SLEEP_ON_KEY() \
    00138         do{\
    00139             EIMSK |= _BV(INT6);\
    00140             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00141             sleep_mode();\
    00142             EIMSK &= ~_BV(INT6);\
    00143         } while(0)
    00144
    00145 #define SLEEP_ON_KEY_vect INT6_vect
    00146
    00147 /*=== Host Interface ================================================*/
    00154 #define HIF_TYPE (HIF_UART_1)
    00155
    00156 /*=== TIMER Interface ===============================================*/
    00164 #define HWTMR_PRESCALE  (1)
    00165 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00166 #define HWTIMER_TICK_NB (0xFFFFUL+1)
    00167 #define HWTIMER_REG     (TCNT1)
    00168 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00169 #define TIMER_POOL_SIZE (4)
    00170 #define TIMER_INIT() \
    00171     do{ \
    00172         TCCR1B |= (_BV(CS10));\
    00173         TIMSK1 |= _BV(TOIE1); \
    00174     }while(0)
    00175 #define TIMER_IRQ_vect  TIMER1_OVF_vect
    00176
    00177
    00178 /*=== OSCCAL tuning =================================================*/
    00179
    00180 #ifndef TUNED_OSCCAL
    00181 # define TUNED_OSCCAL (0xbf)  /* default is 0xb1, but @2.9V 0xbf is better */
    00182 #endif
    00183 #endif /* BOARD_WDBA1281_H*/