# xmpl_trx_base.c - Using Basic Transceiver Access Functions

This example illustrates the use of the basic radio transceiver access functions. It can be used to test a new board definition.

    /* $Id: xmpl_trx_base.c,v 1.8 2009/12/22 16:47:10 joerg_wunsch Exp $ */
    /* Example for accessing the transceiver */

    #include "board.h"
    #include "transceiver.h"
    #include "ioutil.h"
    #include "xmpl.h"

    static volatile trx_regval_t irq_cause;

    int main(void)
    {
    static volatile trx_regval_t rval;

        /* This will stop the application before initializing the radio transceiver
         * (ISP issue with MISO pin, see FAQ)
         */
        trap_if_key_pressed();

        /* init peripherals */
        LED_INIT();
        trx_io_init(SPI_RATE_1_2);
        LED_SET_VALUE(LED_MAX_VALUE);
        LED_SET_VALUE(0);

        /* Step 1: reset transceiver */
        DELAY_US(TRX_INIT_TIME_US);
        TRX_RESET_LOW();
        TRX_SLPTR_LOW();
        DELAY_US(TRX_RESET_TIME_US);
        TRX_RESET_HIGH();
        LED_SET_VALUE(1);
        DELAY_MS(10);

        /* Step 2: check if correct transceiver is present
         * verify if the part and version ID's are correct.
         */
        rval = trx_reg_read(RG_PART_NUM);
        ERR_CHECK(RADIO_PART_NUM != rval);

        rval = trx_reg_read(RG_VERSION_NUM);
        ERR_CHECK_DIAG(RADIO_VERSION_NUM !=rval,2);

        /* Step 3: try a write command on an arbitrary RW register.
         */
        trx_reg_write(RG_IEEE_ADDR_0,42);
        rval = trx_reg_read(RG_IEEE_ADDR_0);
        ERR_CHECK_DIAG((42!=rval),3);

        /* Step 4: go to state TRX_OFF
         * bring the transceiver in state TRX_OFF and verify it.
         */
        trx_reg_write(RG_TRX_STATE, CMD_TRX_OFF);
        DELAY_US(TRX_INIT_TIME_US);
        DELAY_MS(1000);
        rval = trx_bit_read(SR_TRX_STATUS);
        ERR_CHECK_DIAG((TRX_OFF!=rval),4);

        /* Step 5: check SRAM access */

        /* Step 6: check IRQ
         * enable PLL-LOCK IRQ and transceiver IRQ at MCU
         * switch to PLL_ON state (which causes lock IRQ)
         * wait until the interrupt happened
         */
        trx_reg_write(RG_IRQ_MASK, TRX_IRQ_PLL_LOCK);
        irq_cause = 0;
        sei();

        trx_reg_write(RG_TRX_STATE,CMD_PLL_ON);

        DELAY_US(TRX_PLL_LOCK_TIME_US);
        DELAY_MS(1000);
        //ERR_CHECK_DIAG(irq_cause != TRX_IRQ_PLL_LOCK,6);
        ERR_CHECK_DIAG(irq_cause != 0,10);

        /* done */
        LED_SET_VALUE(0);
        while(1)
        {
            WAIT500MS();
            LED_TOGGLE(0);
        }
    }

    #if defined(TRX_IF_RFA1)
    ISR(TRX24_PLL_LOCK_vect)
    {
        irq_cause |= TRX_IRQ_PLL_LOCK;
    }
    #else
    ISR(TRX_IRQ_vect)
    {
        /* reading IRQ_STATUS acknowledges the interrupt */
        irq_cause |= trx_reg_read(RG_IRQ_STATUS);
        LED_SET(1);
    }
    #endif

    /* EOF */