# Radio Constants
[General Constants]

## Defines
#define | MOD_BPSK_20 (0)
#define | MOD_BPSK_40 (1)
#define | MOD_OQPSK_100 (2)
#define | MOD_OQPSK_1000 (7)
#define | MOD_OQPSK_200 (3)
#define | MOD_OQPSK_2000 (8)
#define | MOD_OQPSK_250 (4)
#define | MOD_OQPSK_400 (5)
#define | MOD_OQPSK_500 (6)
#define | RADIO_AT86RF212 (4)
#define | RADIO_AT86RF230 (1)
#define | RADIO_AT86RF230A (RADIO_AT86RF230)
#define | RADIO_AT86RF230B (2)
#define | RADIO_AT86RF231 (3)
#define | RADIO_ATMEGA128RFA1_A (5)
#define | RADIO_ATMEGA128RFA1_B (6)
#define | RADIO_ATMEGA128RFA1_C (7)
#define | RADIO_ATMEGA128RFA1_D (8)
#define | RADIO_BAND_2400 (4)
#define | RADIO_BAND_700 (1)
#define | RADIO_BAND_800 (2)
#define | RADIO_BAND_900 (3)

## Define Documentation

#define MOD_BPSK_20 (0)

PHY modulation BPSK, 20 kbit/s

Definition at line 147 of file const.h.

#define MOD_BPSK_40 (1)

PHY modulation BPSK, 40 kbit/s

Definition at line 148 of file const.h.

#define MOD_OQPSK_100 (2)

PHY modulation O-QPSK, 100 kbit/s

Definition at line 149 of file const.h.

#define MOD_OQPSK_1000 (7)

PHY modulation O-QPSK, 1000 kbit/s

Definition at line 154 of file const.h.

#define MOD_OQPSK_200 (3)

PHY modulation O-QPSK, 200 kbit/s

Definition at line 150 of file const.h.

#define MOD_OQPSK_2000 (8)

PHY modulation O-QPSK, 2000 kbit/s

Definition at line 155 of file const.h.

#define MOD_OQPSK_250 (4)

PHY modulation O-QPSK, 250 kbit/s

Definition at line 151 of file const.h.

#define MOD_OQPSK_400 (5)

PHY modulation O-QPSK, 400 kbit/s

Definition at line 152 of file const.h.

#define MOD_OQPSK_500 (6)

PHY modulation O-QPSK, 500 kbit/s

Definition at line 153 of file const.h.

#define RADIO_AT86RF212 (4)

Identifier for radio AT86RF212

Definition at line 135 of file const.h.

#define RADIO_AT86RF230 (1)

Identifier for radio AT86RF230

Definition at line 131 of file const.h.

#define RADIO_AT86RF230A (RADIO_AT86RF230)

Identifier for radio AT86RF230 Rev A

Definition at line 132 of file const.h.

#define RADIO_AT86RF230B (2)

Identifier for radio AT86RF230 Rev B

Definition at line 133 of file const.h.

#define RADIO_AT86RF231 (3)

Identifier for radio AT86RF231

Definition at line 134 of file const.h.

#define RADIO_ATMEGA128RFA1_A (5)

Identifier for radio ATmega128RFA1 Rev. A

Definition at line 136 of file const.h.

#define RADIO_ATMEGA128RFA1_B (6)

Identifier for radio ATmega128RFA1 Rev. B

Definition at line 137 of file const.h.

#define RADIO_ATMEGA128RFA1_C (7)

Identifier for radio ATmega128RFA1 Rev. C

Definition at line 138 of file const.h.

#define RADIO_ATMEGA128RFA1_D (8)

Identifier for radio ATmega128RFA1 Rev. D

Definition at line 139 of file const.h.

#define RADIO_BAND_2400 (4)

2.4GHz frequency band (international)

Definition at line 144 of file const.h.

#define RADIO_BAND_700 (1)

700MHz frequency band (china)

Definition at line 141 of file const.h.

#define RADIO_BAND_800 (2)

868MHz frequency band (europe)

Definition at line 142 of file const.h.

#define RADIO_BAND_900 (3)

900MHz frequency band (north america)

Definition at line 143 of file const.h.