# Setup on Windows

(back)

1. download the µracoli source package and unpack it
2. open a command shell window with `cmd.exe`
3. change to the to top directory
   `cd /d z:/mysrc/uracoli-ZZZ`
4. build the sniffer application
   `scons a[PLF]`
   ``[PLF] is the name of your target plattform (see `"scons help"`)
5. program your target plattform with the application `"sniffer_[PLF].hex"`, e.g. with AvrStudio
6. verify, that the fuses of the MCU match the predfined values in grpBoard.
7. start wireshark
8. enter the interface name `\\.\pipe\foo` as life capture interface.
9. start the application ieee802154.py
   `python Contrib/PacketCapture/ieee802154.py -p COM12 -i foo`
10. if erything worked well until here, you will see in the cmd shell window:

        uracoli sniffer to wireshark bridge V0.1.0
         OPTS:   -v -p /dev/ttyUSB0 -i foo
         INPUT:  COM12, channel: 15
         OUTPUT: foo

        + waiting for somebody to open the pipe

11. in wireshark select "Capture -> Start" from the menu of The background of wireshark turns white.
12. in the command shell window type `"chan X"`, to select the channel you want to watch.
13. .... now start sending packages in your WSN