Data Structures | Defines

# board.h File Reference

Interface for Board Definitions. More...

Go to the source code of this file.

## Data Structures
struct | node_config_t
## Defines
#define | DBG_CLR() do{}while(0)
#define | DBG_INIT() do{}while(0)
#define | DBG_SET() do{}while(0)
#define | DBG_TOGGLE() do{}while(0)
#define | DELAY_MS(x) _delay_ms(x)
| Macro for delays with ms resolution.
#define | DELAY_US(x) _delay_ms(x/1000.0)
| Macro for delays with us resolution.
#define | DI_TRX_IRQ disable_all_trx_irqs
#define | EI_TRX_IRQ enable_all_trx_irqs
#define | HIF_DEFAULT_BAUDRATE (9600)
#define | HIF_IO_ENABLE() do{}while(0)
#define | HIF_TYPE (HIF_NONE)
#define | HIF_TYPE_IS_UART ((HIF_TYPE >= HIF_UART_0) && ( HIF_TYPE <= HIF_UART_1))
#define | HIF_TYPE_IS_USB ((HIF_TYPE == HIF_FT245) || (HIF_TYPE == HIF_AT90USB))
#define | NO_HIF (1)
#define | PULLUP_KEYS (0)
#define | SLEEP_ON_IDLE()
#define | TRX_RESET_HIGH() PORT_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_INIT() DDR_TRX_RESET |= MASK_TRX_RESET
#define | TRX_RESET_LOW() PORT_TRX_RESET &= ~MASK_TRX_RESET
#define | TRX_SLPTR_HIGH() PORT_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_INIT() DDR_TRX_SLPTR |= MASK_TRX_SLPTR
#define | TRX_SLPTR_LOW() PORT_TRX_SLPTR &= ~MASK_TRX_SLPTR

## Detailed Description

Interface for Board Definitions.