Defines

# board_museIIrfa.h File Reference

MuseII RFA. More...

Go to the source code of this file.

## Defines
#define | BOARD_NAME "museIIrfa"
#define | BOARD_TYPE BOARD_MUSEIIRFA
#define | HIF_TYPE HIF_NONE
#define | HWTIMER_REG (TCNT1)
#define | HWTIMER_TICK ((1.0*HWTMR_PRESCALE)/F_CPU)
#define | HWTIMER_TICK_NB (0xFFFFUL)
#define | HWTMR_PRESCALE (1)
#define | LED_ANODE_bp (3)
#define | LED_CATHODE_bp (4)
#define | LED_DDR DDRE
#define | LED_MASK (0x18)
#define | LED_NUMBER (2)
#define | LED_PIN PINE
#define | LED_PORT PORTE
#define | LED_SHIFT (3)
#define | LEDS_INVERSE (0)
#define | NO_KEYS (1)
#define | RADIO_TYPE (RADIO_ATMEGA128RFA1_D)
#define | TIMER_INIT()
#define | TIMER_IRQ_vect TIMER1_OVF_vect
#define | TIMER_POOL_SIZE (4)
#define | TIMER_TICK (HWTIMER_TICK_NB * HWTIMER_TICK)
#define | TRX_RESET_HIGH() do { TRXPR |= (1<<TRXRST); } while (0)
#define | TRX_RESET_LOW() do { TRXPR &= ~(1<<TRXRST); } while (0)
#define | TRX_SLPTR_HIGH() do { TRXPR |= (1<<SLPTR); } while (0)
#define | TRX_SLPTR_LOW() do { TRXPR &= ~(1<<SLPTR); } while (0)
#define | TRX_TSTAMP_REG TCNT1

## Detailed Description

MuseII RFA.

Build Options

## Define Documentation

#define LED_ANODE_bp (3)

LED anode bit position

#define LED_CATHODE_bp (4)

LED cathode bit position

#define LED_DDR DDRE

DDR register for LEDs

#define LED_MASK (0x18)

MASK value for LEDs (msb aligned)

#define LED_NUMBER (2)

number of LEDs for this board

#define LED_PIN PINE

PIN register for LEDs

#define LED_PORT PORTE

PORT register for LEDs

#define LED_SHIFT (3)

SHIFT value for LEDs

#define LEDS_INVERSE (0)

= 1, if low level at port means LED on

#define NO_KEYS (1)

if defined, no KEYS are connected

#define TIMER_INIT | ( |  | ) |

Value:

    do{ \
            TCCR1B |= ((1<<CS10)); \
            TIMSK1 |= (1<<TOIE1); \
        }while(0)

#define TRX_TSTAMP_REG TCNT1

timestamp register for RX_START event