# board_cbb2xx.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2011 Axel Wachtler, Daniel Thiele
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id$ */
    00058 #ifndef BOARD_CBB2XX_H
    00059 #define BOARD_CBB2XX_H
    00060
    00061 #if defined(cbb230)
    00062 # define BOARD_TYPE BOARD_CBB230
    00063 # define BOARD_NAME "cbb230"
    00064 # define RADIO_TYPE (RADIO_AT86RF230A)
    00065 #elif defined(cbb230b)
    00066 # define BOARD_TYPE BOARD_CBB230B
    00067 # define BOARD_NAME "cbb230b"
    00068 # define RADIO_TYPE (RADIO_AT86RF230B)
    00069 #elif defined(cbb231)
    00070 # define BOARD_TYPE BOARD_CBB231
    00071 # define BOARD_NAME "cbb231"
    00072 # define RADIO_TYPE (RADIO_AT86RF231)
    00073 #elif defined(cbb212)
    00074 # define BOARD_TYPE BOARD_CBB212
    00075 # define BOARD_NAME "cbb212"
    00076 # define RADIO_TYPE (RADIO_AT86RF212)
    00077 #elif defined(cbb232)
    00078 # define BOARD_TYPE BOARD_CBB232
    00079 # define BOARD_NAME "cbb232"
    00080 # define RADIO_TYPE (RADIO_AT86RF232)
    00081 #elif defined(cbb233)
    00082 # define BOARD_TYPE BOARD_CBB233
    00083 # define BOARD_NAME "cbb233"
    00084 # define RADIO_TYPE (RADIO_AT86RF233)
    00085 #endif
    00086
    00087 #ifndef DEFAULT_SPI_RATE
    00088 # define DEFAULT_SPI_RATE  (SPI_RATE_1_2)
    00089 #endif
    00090
    00091 /*=== Hardware Components ============================================*/
    00092
    00093 /*=== TRX pin access macros ==========================================*/
    00094
    00095 #define PORT_TRX_RESET  PORTC
    00096 #define MASK_TRX_RESET  (_BV(0))
    00098 #define TRX_RESET_INIT() PORT_TRX_RESET.DIRSET = MASK_TRX_RESET
    00099 #define TRX_RESET_HIGH() PORT_TRX_RESET.OUTSET = MASK_TRX_RESET
    00100 #define TRX_RESET_LOW()  PORT_TRX_RESET.OUTCLR = MASK_TRX_RESET
    00102 #define PORT_TRX_SLPTR  PORTC
    00103 #define MASK_TRX_SLPTR  (_BV(3))
    00106 #define TRX_SLPTR_INIT() PORT_TRX_SLPTR.DIRSET = MASK_TRX_SLPTR
    00107
    00108 #define TRX_SLPTR_HIGH() PORT_TRX_SLPTR.OUTSET = MASK_TRX_SLPTR
    00109
    00110 #define TRX_SLPTR_LOW()  PORT_TRX_SLPTR.OUTCLR = MASK_TRX_SLPTR
    00111
    00112
    00113 /*=== IRQ access macros ==============================================*/
    00114 # define TRX_IRQ_vect    PORTC_INT0_vect
    00115 # define TRX_IRQ         _BV(2)
    00121 # define TRX_IRQ_INIT()  do{\
    00122                             PORTC.INT0MASK = TRX_IRQ; \
    00123                             PORTC.INTCTRL = PORT_INT0LVL_HI_gc; \
    00124                             PMIC.CTRL |= PMIC_HILVLEN_bm;\
    00125                           } while(0)
    00126
    00128 #define DI_TRX_IRQ() {PORTC.INT0MASK &= ~TRX_IRQ;}
    00129
    00131 #define EI_TRX_IRQ() {PORTC.INT0MASK |= TRX_IRQ;}
    00132
    00137 #define TRX_TSTAMP_REG TCD0.CNT
    00138
    00139 /*=== SPI access macros ==============================================*/
    00140 #define PORT_SPI (PORTC)
    00142 #define SPI_MOSI _BV(5)
    00143 #define SPI_MISO _BV(6)
    00144 #define SPI_SCK  _BV(7)
    00145 #define SPI_SS   _BV(4)
    00147 #define SPI_DATA_REG SPIC.DATA
    00153 static inline void SPI_INIT(uint8_t spirate)
    00154 {
    00155     /* first configure SPI Port, then SPCR */
    00156     PORT_SPI.OUTSET = SPI_SCK | SPI_SS;
    00157     PORT_SPI.DIRSET = SPI_MOSI | SPI_SCK | SPI_SS;
    00158     PORT_SPI.DIRCLR = SPI_MISO;
    00159
    00160     SPIC.CTRL = SPI_ENABLE_bm | SPI_MASTER_bm;
    00161
    00162     SPIC.CTRL |= (spirate & 0x03);
    00163     SPIC.CTRL |= ((spirate << 5) & 0x80); /* CLK2X */
    00164 }
    00165
    00167 #define SPI_SELN_LOW()       uint8_t sreg = SREG; cli(); PORT_SPI.OUTCLR = SPI_SS
    00168
    00169 #define SPI_SELN_HIGH()      PORT_SPI.OUTSET = SPI_SS; SREG = sreg
    00170
    00171 #define SPI_WAITFOR()        do { while((SPIC.STATUS & SPI_IF_bm) == 0);} while(0)
    00172
    00173
    00174 /*=== LED access macros ==============================================*/
    00175 #define LED_PORT     PORTB_OUT
    00176 #define LED_DDR      PORTB_DIR
    00177 #define LED_MASK     (0x07)
    00178 #define LED_SHIFT    (0)
    00179 #define LEDS_INVERSE (0)
    00180 #define LED_NUMBER   (3)
    00181
    00182 /*=== KEY access macros ==============================================*/
    00183 #define PORT_KEY     PORTB_OUT
    00184 #define PIN_KEY      PORTB_IN
    00185 #define DDR_KEY      PORTB_DIR
    00186 #define MASK_KEY     (0x08)
    00187 #define SHIFT_KEY    (3)
    00188 #define INVERSE_KEYS (1)
    00189
    00190 #define KEY_INIT() do{ PORTB_PIN3CTRL = PORT_OPC_PULLUP_gc; DDR_KEY &= ~MASK_KEY; }while(0)
    00191
    00192 #define SLEEP_ON_KEY_INIT() do{}while(0)
    00193 #define SLEEP_ON_KEY() \
    00194         do{\
    00195         } while(0)
    00196
    00197 #define SLEEP_ON_KEY_vect PORTB_INT0_vect
    00198
    00199 /*=== Host Interface ================================================*/
    00200 #define HIF_TYPE (HIF_UART_0)
    00201
    00202 /*=== TIMER Interface ===============================================*/
    00203 #define HWTMR_PRESCALE  (1)
    00204 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00205 #define HWTIMER_TICK_NB (0xFFFFUL)
    00206 #define HWTIMER_REG     (TCD0.CNT)
    00207 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00208 #define TIMER_POOL_SIZE (4)
    00209 #define TIMER_INIT() \
    00210     do{ \
    00211         TCD0.CTRLA = TC_CLKSEL_DIV1_gc; \
    00212         TCD0.INTFLAGS |= TC0_OVFIF_bm; \
    00213         TCD0.INTCTRLA = TC_OVFINTLVL_HI_gc; \
    00214     }while(0)
    00215 #define TIMER_IRQ_vect   TCD0_OVF_vect
    00216
    00217 #endif /* BOARD_CBB2XX_H */