# board_any.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2010 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id$ */
    00102 #if defined(any900)
    00103 # define BOARD_TYPE (BOARD_ANY900)
    00104 # define BOARD_NAME "any900"
    00105 # define RADIO_TYPE (RADIO_AT86RF212)
    00106 #elif defined(any2400)
    00107 # define BOARD_TYPE (BOARD_ANY2400)
    00108 # define BOARD_NAME "any2400"
    00109 # define RADIO_TYPE (RADIO_AT86RF230)
    00110 #elif defined(any900st)
    00111 # define BOARD_TYPE (BOARD_ANY900ST)
    00112 # define BOARD_NAME "any900st"
    00113 # define RADIO_TYPE (RADIO_AT86RF212)
    00114 #elif defined(any2400st)
    00115 # define BOARD_TYPE (BOARD_ANY2400ST)
    00116 # define BOARD_NAME "any2400st"
    00117 # define RADIO_TYPE (RADIO_AT86RF230)
    00118 #endif
    00119
    00120 #ifndef BOARD_ANY_H
    00121 #define BOARD_ANY_H
    00122
    00123
    00124 /*=== Compile time parameters ========================================*/
    00125
    00126 /*=== radio interface definition =====================================*/
    00127 #include "base_zdma1281.h"
    00128
    00129 /*=== LED access macros ==============================================*/
    00130 #define LED_PORT PORTB
    00131 #define LED_DDR  DDRB
    00132 #define LED_MASK 0xe0
    00133 #define LED_SHIFT     (5)
    00134 #define LEDS_INVERSE  (0)
    00135 #define LED_NUMBER    (3)
    00137 /*=== KEY access macros ==============================================*/
    00138 #define PORT_KEY PORTE
    00139 #define PIN_KEY  PINE
    00140 #define DDR_KEY  DDRE
    00141
    00142 #define MASK_KEY     (0xc0)
    00143 #define SHIFT_KEY    (6)
    00144 #define INVERSE_KEYS (1)
    00145 #define PULLUP_KEYS  (1)
    00146
    00147 #define SLEEP_ON_KEY_INIT() do{}while(0)
    00148 #define SLEEP_ON_KEY() \
    00149         do{\
    00150             EIMSK |= _BV(INT6);\
    00151             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00152             sleep_mode();\
    00153             EIMSK &= ~_BV(INT6);\
    00154         } while(0)
    00155
    00156 #define SLEEP_ON_KEY_vect INT6_vect
    00157
    00158 /*=== Host Interface ================================================*/
    00159
    00166 #define HIF_TYPE (HIF_UART_1)
    00167
    00168 /*=== TIMER Interface ===============================================*/
    00176 #define HWTMR_PRESCALE  (1)
    00177 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00178 #define HWTIMER_TICK_NB (0xFFFFUL+1)
    00179 #define HWTIMER_REG     (TCNT1)
    00180 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00181 #define TIMER_POOL_SIZE (4)
    00182 #define TIMER_INIT() \
    00183     do{ \
    00184         TCCR1B |= (_BV(CS10));\
    00185         TIMSK1 |= _BV(TOIE1); \
    00186     }while(0)
    00187 #define TIMER_IRQ_vect  TIMER1_OVF_vect
    00188
    00189 #endif /* BOARD_ANY_H*/