# board_wdba1281.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2008 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id$ */
    00101 #if defined(mnb900)
    00102 # define BOARD_TYPE (BOARD_MNB900)
    00103 # define BOARD_NAME "mnb900"
    00104 # define RADIO_TYPE (RADIO_AT86RF212)
    00105 #elif defined(wdba1281)
    00106 # define BOARD_TYPE (BOARD_WDBA1281)
    00107 # define BOARD_NAME "wdba1281"
    00108 # define RADIO_TYPE (RADIO_AT86RF230)
    00109 #elif defined(bitbean)
    00110 # define BOARD_TYPE (BOARD_BITBEAN)
    00111 # define BOARD_NAME "bitbean"
    00112 # define RADIO_TYPE (RADIO_AT86RF230)
    00113 #endif
    00114
    00115 #ifndef BOARD_WDBA1281_H
    00116 #define BOARD_WDBA1281_H
    00117
    00118 /*=== Compile time parameters ========================================*/
    00119
    00120 /*=== radio interface definition =====================================*/
    00121 #include "base_zdma1281.h"
    00122
    00123 /*=== LED access macros ==============================================*/
    00124 #define LED_PORT PORTB
    00125 #define LED_DDR  DDRB
    00126 #define LED_MASK 0xe0
    00127 #define LED_SHIFT     (5)
    00128 #define LEDS_INVERSE  (0)
    00129 #define LED_NUMBER    (3)
    00131 /*=== KEY access macros ==============================================*/
    00132 #define PORT_KEY PORTE
    00133 #define PIN_KEY  PINE
    00134 #define DDR_KEY  DDRE
    00135
    00136
    00137 #if defined(bitbean)
    00138 # define MASK_KEY     (0x80)
    00139 # define SHIFT_KEY    (7)
    00140 # define INVERSE_KEYS (1)
    00141 # define PULLUP_KEYS  (1)
    00142
    00143 # define SLEEP_ON_KEY_INIT() do{}while(0)
    00144 # define SLEEP_ON_KEY() \
    00145         do{\
    00146             EIMSK |= _BV(INT7);\
    00147             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00148             sleep_mode();\
    00149             EIMSK &= ~_BV(INT7);\
    00150         } while(0)
    00151
    00152 # define SLEEP_ON_KEY_vect INT7_vect
    00153 #else
    00154 # define MASK_KEY     (0xc0)
    00155 # define SHIFT_KEY    (6)
    00156 # define INVERSE_KEYS (1)
    00157 # define PULLUP_KEYS  (1)
    00158
    00159 # define SLEEP_ON_KEY_INIT() do{}while(0)
    00160 # define SLEEP_ON_KEY() \
    00161         do{\
    00162             EIMSK |= _BV(INT6);\
    00163             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00164             sleep_mode();\
    00165             EIMSK &= ~_BV(INT6);\
    00166         } while(0)
    00167
    00168 # define SLEEP_ON_KEY_vect INT6_vect
    00169 #endif
    00170
    00171 /*=== Host Interface ================================================*/
    00178 #define HIF_TYPE (HIF_UART_1)
    00179 #if defined(bitbean)
    00180
    00190 # define HIF_IO_ENABLE() \
    00191    do{ DDRG |= 0x07; PORTG |= 0x01;}while(0);
    00192 #endif
    00193 /*=== TIMER Interface ===============================================*/
    00201 #define HWTMR_PRESCALE  (1)
    00202 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00203 #define HWTIMER_TICK_NB (0xFFFFUL+1)
    00204 #define HWTIMER_REG     (TCNT1)
    00205 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00206 #define TIMER_POOL_SIZE (4)
    00207 #define TIMER_INIT() \
    00208     do{ \
    00209         TCCR1B |= (_BV(CS10));\
    00210         TIMSK1 |= _BV(TOIE1); \
    00211     }while(0)
    00212 #define TIMER_IRQ_vect  TIMER1_OVF_vect
    00213
    00214 #endif /* BOARD_WDBA1281_H*/