Data Fields

# p2p_ping_cnf_t Struct Reference

## Data Fields
char | appname [8]
char | boardname []
uint16_t | crc
p2p_error_t | errno
p2p_hdr_t | hdr
p2p_status_t | status
uint8_t | version

## Detailed Description

Frame structure for P2P_PING_CNF.

## Field Documentation

char p2p_ping_cnf_t::appname[8]

application identification string

char p2p_ping_cnf_t::boardname[]

board identification string

uint16_t p2p_ping_cnf_t::crc

checksum of received data (only used from WIBO)

p2p_error_t p2p_ping_cnf_t::errno

current error code

p2p_status_t p2p_ping_cnf_t::status

application status

uint8_t p2p_ping_cnf_t::version

software version