lwIP 2.1.0 Lightweight IP stack

Macros | Functions
httpd.c File Reference
`#include "lwip/init.h"`
`#include "lwip/apps/httpd.h"`
`#include "lwip/debug.h"`
`#include "lwip/stats.h"`
`#include "lwip/apps/fs.h"`
`#include "httpd_structs.h"`
`#include "lwip/def.h"`
`#include "lwip/altcp.h"`
`#include "lwip/altcp_tcp.h"`
`#include "lwip/altcp_tls.h"`
`#include "path/to/my/lwip_hooks.h"`
`#include <string.h>`
`#include <stdlib.h>`
`#include <stdio.h>`

## Macros
#define | MIN_REQ_LEN 7
#define | HTTP_IS_DATA_VOLATILE(hs) (HTTP_IS_DYNAMIC_FILE(hs) ? TCP_WRITE_FLAG_COPY : 0)
#define | HTTP_IS_HDR_VOLATILE(hs, ptr) 0

## Functions
void | httpd_post_data_recved (void *connection, u16_t recved_len)
void | httpd_init (void)
void | httpd_inits (struct altcp_tls_config *conf)
void | http_set_ssi_handler (tSSIHandler ssi_handler, const char **tags, int num_tags)
void | http_set_cgi_handlers (const tCGI *cgis, int num_handlers)

## Detailed Description

LWIP HTTP server implementation

## Macro Definition Documentation

## ◆ HTTP_IS_DATA_VOLATILE

#define HTTP_IS_DATA_VOLATILE | ( |  | hs | ) | (HTTP_IS_DYNAMIC_FILE(hs) ? TCP_WRITE_FLAG_COPY : 0)

tcp_write does not have to copy data when sent from rom-file-system directly

## ◆ HTTP_IS_HDR_VOLATILE

#define HTTP_IS_HDR_VOLATILE | ( |  | hs,
|  |  | ptr
| ) |  | 0

Default: dynamic headers are sent from ROM (non-dynamic headers are handled like file data)

## ◆ MIN_REQ_LEN

#define MIN_REQ_LEN 7

Minimum length for a valid HTTP/0.9 request: "GET /\r\n" -> 7 bytes