lwIP 2.1.0 Lightweight IP stack

Macros
NO_SYS
lwIP » Options (lwipopts.h) » Infrastructure

## Macros
#define | NO_SYS 0

## Detailed Description

## Macro Definition Documentation

## ◆ NO_SYS

#define NO_SYS 0

NO_SYS==1: Use lwIP without OS-awareness (no thread, semaphores, mutexes or mboxes). This means threaded APIs cannot be used (socket, netconn, i.e. everything in the 'api' folder), only the callback-style raw API is available (and you have to watch out for yourself that you don't access lwIP functions/structures from more than one context at a time!)