lwIP 2.1.3 Lightweight IP stack

Data Fields
mdns_service Struct Reference

## Data Fields
struct mdns_domain | txtdata
char | name [63+1]
char | service [63+1]
service_get_txt_fn_t | txt_fn
u32_t | dns_ttl
u16_t | proto
u16_t | port

## Detailed Description

Description of a service

## Field Documentation

## ◆ dns_ttl

u32_t mdns_service::dns_ttl

TTL in seconds of SRV/TXT replies

## ◆ name

char mdns_service::name[63+1]

Name of service, like 'myweb'

## ◆ port

u16_t mdns_service::port

Port of the service

## ◆ proto

u16_t mdns_service::proto

Protocol, TCP or UDP

## ◆ service

char mdns_service::service[63+1]

Type of service, like '_http'

## ◆ txt_fn

service_get_txt_fn_t mdns_service::txt_fn

Callback function and userdata to update txtdata buffer

## ◆ txtdata

struct mdns_domain mdns_service::txtdata

TXT record to answer with

The documentation for this struct was generated from the following file:

- src/apps/mdns/mdns.c