- Main Page
- Related Pages
- Modules
- Data Structures
- Files

# board_ict_11.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2009 Karl Fessel, Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_ict_11.h,v 1.2 2009/06/30 19:27:22 awachtler Exp $ */
    00082 #if defined(ics230_11)
    00083 # define BOARD_NAME_ICT230_11 "icstick230"
    00084 # define BOARD_TYPE  (ICSTICK_RF230)
    00085 #elif defined(icm230_11)
    00086 # define BOARD_NAME_ICT230_11 "icmodule230"
    00087 # define BOARD_TYPE  (ICMODULE_RF230)
    00088 #endif
    00089
    00090 #ifndef BOARD_ICT230_11_H
    00091 #define BOARD_ICT230_11_H
    00092
    00093
    00094 #define BOARD_NAME  BOARD_NAME_ICT230_11
    00095
    00096 /*=== Compile time parameters ========================================*/
    00097 #ifndef MAX_FRAME_SIZE
    00098 # define MAX_FRAME_SIZE (127)
    00099 #endif
    00100
    00101 #ifndef DEFAULT_SPI_RATE
    00102 # define DEFAULT_SPI_RATE  (SPI_RATE_1_4)
    00103 #endif
    00104
    00105 /*=== Hardware Components ============================================*/
    00106 #define CPU_TYPE   (CPU_M1281)
    00107 #define RADIO_TYPE (RADIO_AT86RF230B)
    00109 /*=== TRX pin access macros ==========================================*/
    00110 #include "base_rdk230.h"
    00111 #define CUSTOM_RESET_TIME_MS (10)
    00113 /*=== LED access macros ==============================================*/
    00114
    00115 /* stick settings */
    00116 #if BOARD_TYPE == ICSTICK_RF230
    00117 # define LED_PORT      PORTG
    00118 # define LED_DDR       DDRG
    00119 # define LED_MASK      (0x20)
    00120 # define LED_SHIFT     (5)
    00121 # define LEDS_INVERSE  (1)
    00122 # define LED_NUMBER    (1)
    00123 #elif BOARD_TYPE == ICMODULE_RF230
    00124 # define LED_PORT      PORTD
    00125 # define LED_DDR       DDRD
    00126 # define LED_MASK      (0xc0)
    00127 # define LED_SHIFT     (6)
    00128 # define LEDS_INVERSE  (1)
    00129 # define LED_NUMBER    (2)
    00130 #endif
    00131
    00132
    00133 /*=== KEY access macros ==============================================*/
    00134 #if BOARD_TYPE == ICSTICK_RF230
    00135 # define NO_KEYS (1)
    00136 #elif BOARD_TYPE == ICMODULE_RF230
    00137 # define PORT_KEY     PORTD
    00138 # define PIN_KEY      PIND
    00139 # define DDR_KEY      DDRD
    00140 # define MASK_KEY     (0x01)
    00141 # define SHIFT_KEY    (0)
    00142 # define INVERSE_KEYS (1)
    00143 # define PULLUP_KEYS  (1)
    00144 #endif
    00145
    00146 /*=== Host Interface ================================================*/
    00147 #define HIF_TYPE    HIF_UART_1
    00148
    00149
    00150 /*=== TIMER Interface ===============================================*/
    00151 #define HWTMR_PRESCALE  (1)
    00152 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00153 #define HWTIMER_TICK_NB (0xFFFFUL)
    00154 #define HWTIMER_REG     (TCNT1)
    00155 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00156 #define TIMER_POOL_SIZE (4)
    00157 #define TIMER_INIT() \
    00158     do{ \
    00159         TCCR1B |= (_BV(CS10)); \
    00160         TIMSK1 |= _BV(TOIE1); \
    00161     }while(0)
    00162
    00163 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00164
    00165 /*=== OSCCAL tuning =================================================*/
    00166
    00167 #ifndef TUNED_OSCCAL
    00168 # define TUNED_OSCCAL (0xbf)  /* default is 0xb1, but @2.9V 0xbf is better */
    00169 #endif
    00170 #endif /* BOARD_ICT230_11_H */