- Main Page
- Related Pages
- Modules
- Data Structures
- Files

# board_rdk230.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2007 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_rdk230.h,v 1.14 2009/11/22 19:06:48 awachtler Exp $ */
    00080 #if defined(rdk230)
    00081 # define BOARD_TYPE  RDK_230
    00082 # define BOARD_NAME_RDK230 "rdk230"
    00083 # define RADIO_TYPE (RADIO_AT86RF230A)
    00084 #elif defined(rdk230b)
    00085 # define BOARD_TYPE  RDK_230
    00086 # define BOARD_NAME_RDK230 "rdk230b"
    00087 # define RADIO_TYPE (RADIO_AT86RF230B)
    00088 #elif defined(rdk231)
    00089 # define BOARD_TYPE  RDK_231
    00090 # define BOARD_NAME_RDK230 "rdk231"
    00091 # define RADIO_TYPE (RADIO_AT86RF231)
    00092 #elif defined(rdk212)
    00093 # define BOARD_TYPE  RDK_212
    00094 # define BOARD_NAME_RDK230 "rdk212"
    00095 # define RADIO_TYPE (RADIO_AT86RF212)
    00096 #endif
    00097
    00098 #ifndef BOARD_RDK230_H
    00099 #define BOARD_RDK230_H
    00100
    00101 #define BOARD_NAME  BOARD_NAME_RDK230
    00102
    00103 /*=== Compile time parameters ========================================*/
    00104 #ifndef MAX_FRAME_SIZE
    00105 # define MAX_FRAME_SIZE (127)
    00106 #endif
    00107
    00108 /*=== radio interface definition =====================================*/
    00109 #if BOARD_TYPE == RDK_212 || BOARD_TYPE == RDK_231
    00110 # include "base_rdk2xx.h"
    00111 #else
    00112 # include "base_rdk230.h"
    00113 #endif
    00114
    00115 /*=== LED access macros ==============================================*/
    00116 #define LED_PORT     PORTE
    00117 #define LED_DDR      DDRE
    00118 #define LED_MASK     (0x1c)
    00119 #define LED_SHIFT    (2)
    00120 #define LEDS_INVERSE (1)
    00121 #define LED_NUMBER   (3)
    00122
    00123 /*=== KEY access macros ==============================================*/
    00124 #define PORT_KEY     PORTE
    00125 #define PIN_KEY      PINE
    00126 #define DDR_KEY      DDRE
    00127 #define MASK_KEY     (0x20)
    00128 #define SHIFT_KEY    (5)
    00129 #define INVERSE_KEYS (1)
    00130 #define PULLUP_KEYS  (1)
    00131
    00132 #define SLEEP_ON_KEY_INIT() do{}while(0)
    00133 #define SLEEP_ON_KEY() \
    00134         do{\
    00135             EIMSK |= _BV(INT5);\
    00136             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00137             sleep_mode();\
    00138             EIMSK &= ~_BV(INT5);\
    00139         } while(0)
    00140
    00141 #define SLEEP_ON_KEY_vect INT5_vect
    00142
    00143 /*=== Host Interface ================================================*/
    00144 #define HIF_TYPE (HIF_UART_1)
    00145
    00146 /*=== TIMER Interface ===============================================*/
    00147 #define HWTMR_PRESCALE  (1)
    00148 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00149 #define HWTIMER_TICK_NB (0xFFFFUL)
    00150 #define HWTIMER_REG     (TCNT1)
    00151 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00152 #define TIMER_POOL_SIZE (4)
    00153 #define TIMER_INIT() \
    00154     do{ \
    00155         TCCR1B |= (_BV(CS10)); \
    00156         TIMSK1 |= _BV(TOIE1); \
    00157     }while(0)
    00158 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00159
    00160 /*=== OSCCAL tuning =================================================*/
    00161
    00162 #ifndef TUNED_OSCCAL
    00163 # define TUNED_OSCCAL (0xbf)  /* default is 0xb1, but @2.9V 0xbf is better */
    00164 #endif
    00165 #endif /* BOARD_RDK230_H*/