- Main Page
- Related Pages
- Modules
- Data Structures
- Files

# board_rbbrfa1.h

Go to the documentation of this file.

    00001 /* Copyright (c) 2009 Axel Wachtler
    00002    All rights reserved.
    00003
    00004    Redistribution and use in source and binary forms, with or without
    00005    modification, are permitted provided that the following conditions
    00006    are met:
    00007
    00008    * Redistributions of source code must retain the above copyright
    00009      notice, this list of conditions and the following disclaimer.
    00010    * Redistributions in binary form must reproduce the above copyright
    00011      notice, this list of conditions and the following disclaimer in the
    00012      documentation and/or other materials provided with the distribution.
    00013    * Neither the name of the authors nor the names of its contributors
    00014      may be used to endorse or promote products derived from this software
    00015      without specific prior written permission.
    00016
    00017    THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
    00018    AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
    00019    IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
    00020    ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE
    00021    LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
    00022    CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
    00023    SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
    00024    INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
    00025    CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
    00026    ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
    00027    POSSIBILITY OF SUCH DAMAGE. */
    00028
    00029 /* $Id: board_rbbrfa1.h,v 1.2 2009/12/25 18:40:49 awachtler Exp $ */
    00063 #if defined(rbb128rfa1)
    00064 # define BOARD_TYPE  RCB_BB_128RFA1
    00065 # define BOARD_NAME "rbb128rfa1"
    00066 # define CPU_TYPE   (CPU_M128RFA1)
    00067 # define RADIO_TYPE (RADIO_ATMEGA128RFA1_C)
    00068 #endif
    00069
    00070 #ifndef BOARD_RBBRFA1_H
    00071 #define BOARD_RBBRFA1_H
    00072
    00073 /*=== Compile time parameters ========================================*/
    00074 #ifndef MAX_FRAME_SIZE
    00075 # define MAX_FRAME_SIZE (127)
    00076 #endif
    00077
    00079 #define TRX_TSTAMP_REG TCNT1
    00080
    00081 /*=== LED access macros ==============================================*/
    00082 #define LED_PORT     PORTE
    00083 #define LED_DDR      DDRE
    00084 #define LED_MASK     (0x1c)
    00085 #define LED_SHIFT    (2)
    00086 #define LEDS_INVERSE (1)
    00087 #define LED_NUMBER   (3)
    00088
    00089 /*=== KEY access macros ==============================================*/
    00090 #define PORT_KEY     PORTE
    00091 #define PIN_KEY      PINE
    00092 #define DDR_KEY      DDRE
    00093 #define MASK_KEY     (0x20)
    00094 #define SHIFT_KEY    (5)
    00095 #define INVERSE_KEYS (1)
    00096 #define PULLUP_KEYS  (1)
    00097
    00098 #define SLEEP_ON_KEY_INIT() do{}while(0)
    00099 #define SLEEP_ON_KEY() \
    00100         do{\
    00101             EIMSK |= _BV(INT5);\
    00102             set_sleep_mode(SLEEP_MODE_PWR_DOWN);\
    00103             sleep_mode();\
    00104             EIMSK &= ~_BV(INT5);\
    00105         } while(0)
    00106
    00107 #define SLEEP_ON_KEY_vect INT5_vect
    00108
    00109 /*=== Host Interface ================================================*/
    00110
    00111 #define HIF_TYPE    HIF_UART_1
    00112
    00113 #define TRX_RESET_LOW()   do { TRXPR &= ~_BV(TRXRST); } while (0)
    00114 #define TRX_RESET_HIGH()  do { TRXPR |= _BV(TRXRST); } while (0)
    00115 #define TRX_SLPTR_LOW()   do { TRXPR &= ~_BV(SLPTR); } while (0)
    00116 #define TRX_SLPTR_HIGH()  do { TRXPR |= _BV(SLPTR); } while (0)
    00117
    00118 /*=== TIMER Interface ===============================================*/
    00119 #define HWTMR_PRESCALE  (1)
    00120 #define HWTIMER_TICK    ((1.0*HWTMR_PRESCALE)/F_CPU)
    00121 #define HWTIMER_TICK_NB (0xFFFFUL)
    00122 #define HWTIMER_REG     (TCNT1)
    00123 #define TIMER_TICK      (HWTIMER_TICK_NB * HWTIMER_TICK)
    00124 #define TIMER_POOL_SIZE (4)
    00125 #define TIMER_INIT() \
    00126     do{ \
    00127         TCCR1B |= (_BV(CS10)); \
    00128         TIMSK1 |= _BV(TOIE1); \
    00129     }while(0)
    00130 #define TIMER_IRQ_vect   TIMER1_OVF_vect
    00131
    00132 /*=== OSCCAL tuning =================================================*/
    00133
    00134 #endif /* BOARD_RBBRFA1_H*/