# const.h File Reference

## Detailed Description

Definitions for General Constants.

Definition in file const.h.

Go to the source code of this file.

## Data Structures
struct | trx_param_t
## Defines
#define | CPU_M1281 (3)
#define | CPU_M1284 (7)
#define | CPU_M1287 (6)
#define | CPU_M128RFA1 (10)
#define | CPU_M16 (2)
#define | CPU_M644P (9)
#define | CPU_M8 (1)
#define | CPU_M88 (8)
#define | CPU_T26 (4)
#define | CPU_T44 (5)
#define | DE_MOD_128RFA1 (29)
#define | FCTL_ACK _BV(5)
#define | FCTL_DATA _BV(0)
#define | FCTL_DST_LONG 0x0c00
#define | FCTL_DST_MASK (FCTL_DST_LONG)
#define | FCTL_DST_SHORT 0x0800
#define | FCTL_IPAN _BV(6)
#define | FCTL_IPAN_MASK (FCTL_IPAN)
#define | FCTL_SRC_LONG 0xc000
#define | FCTL_SRC_MASK (FCTL_SRC_LONG)
#define | FCTL_SRC_SHORT 0x8000
#define | HIF_AT90USB (21)
#define | HIF_FT245 (20)
#define | HIF_NONE (0)
#define | HIF_UART_0 (10)
#define | HIF_UART_1 (11)
#define | ICMODULE_RF230 (43)
#define | ICSTICK_RF230 (42)
#define | ICT_RF230 (41)
#define | LITTLE_GEE_231 (94)
#define | MNB_900 (31)
#define | MOD_BPSK_20 (0)
#define | MOD_BPSK_40 (1)
#define | MOD_OQPSK_100 (2)
#define | MOD_OQPSK_1000 (7)
#define | MOD_OQPSK_200 (3)
#define | MOD_OQPSK_2000 (8)
#define | MOD_OQPSK_250 (4)
#define | MOD_OQPSK_400 (5)
#define | MOD_OQPSK_500 (6)
#define | PSK_212 (13)
#define | PSK_230 (10)
#define | PSK_230B (11)
#define | PSK_231 (12)
#define | RADIO_AT86RF212 (4)
#define | RADIO_AT86RF230 (1)
#define | RADIO_AT86RF230A (RADIO_AT86RF230)
#define | RADIO_AT86RF230B (2)
#define | RADIO_AT86RF231 (3)
#define | RADIO_ATMEGA128RFA1_A (5)
#define | RADIO_ATMEGA128RFA1_B (6)
#define | RADIO_ATMEGA128RFA1_C (7)
#define | RADIO_ATMEGA128RFA1_D (8)
#define | RADIO_BAND_2400 (4)
#define | RADIO_BAND_700 (1)
#define | RADIO_BAND_800 (2)
#define | RADIO_BAND_900 (3)
#define | RAV_LCD (3)
#define | RAV_RF230 (2)
#define | RCB_BB_128RFA1 (24)
#define | RCB_BB_212 (28)
#define | RCB_BB_230 (25)
#define | RCB_BB_230B (26)
#define | RCB_BB_231 (27)
#define | RDK_212 (18)
#define | RDK_230 (15)
#define | RDK_231 (17)
#define | RZ_USB230 (1)
#define | SHORTENUM
#define | SPI_RATE_1_128 (3)
#define | SPI_RATE_1_16 (1)
#define | SPI_RATE_1_2 (4)
#define | SPI_RATE_1_32 (6)
#define | SPI_RATE_1_4 (0)
#define | SPI_RATE_1_64 (2)
#define | SPI_RATE_1_8 (5)
#define | STB_212 (23)
#define | STB_230 (20)
#define | STB_230B (21)
#define | STB_231 (22)
#define | STK500_MEGA16 (92)
#define | STK500_MEGA8 (91)
#define | STK500_TINY26 (93)
#define | TINY_230 (90)
#define | URACOLI_USB_BCD_RELEASE (0x100)
#define | URACOLI_USB_PID (2183)
#define | URACOLI_USB_PRODUCT_NAME L"RZUSBSTICK"
#define | URACOLI_USB_VENDOR_NAME L"URACOLI"
#define | URACOLI_USB_VID (5824)
#define | WDB_A1281 (30)
#define | ZGB_LINK_212 (52)
#define | ZGB_LINK_230 (50)
#define | ZGB_LINK_231 (51)
## Typedefs
typedef uint8_t | ccamode_t
typedef int8_t | channel_t
typedef bool | rxidle_t
typedef int8_t | txpwr_t